(---------------------------------------------------------------------)
(                                                                     )
(    ARTWORK LOG                                                      )
(                                                                     )
(    Drawing          : TWR_MPC8309_32_20111027.brd                   )
(    Software Version : 16.3S033                                      )
(    Date/Time        : Mon Oct 31 10:47:40 2011                      )
(                                                                     )
(---------------------------------------------------------------------)


 ---- Photoplot outline rectangle not found; using drawing extents.



Results from parameter file ...
    DEVICE-TYPE           GERBER_RS274X
    OUTPUT-UNITS          INCHES
    FILM-SIZE             2400000 1600000
    FORMAT                3.5
    ABORT-ON-ERROR        NO
    SCALE                 1
    SUPPRESS-LEAD-ZEROES  YES
    SUPPRESS-TRAIL-ZEROES NO
    SUPPRESS-EQUAL        YES
    UNDEF-APT-CONT        NO


================================================================
     PROCESSING FILM < BOTASSY >
     TO FILE < D:/8309 Rev.B/brd/BOTASSY.art > ...
================================================================

  FILM PARAMETERS :
  ---------------------------------------------------------
  Undefined line width                6.00
  Mirror code                         X
  Rotate angle                        NONE
  Offset x:                           0.00
  Offset y:                           0.00
  Plot negative                       NO
  Suppress unconnected internal pads  NO

    WARNING: 0 width line found at (-1698.54 1871.46)
           ... using undefined line width of 6.00

    WARNING: Multiple 0 width lines; all will be treated the same as the first.
           ... using undefined line width of 6.00

    WARNING: text composed 0 width line found at (-1548.54 -338.54)
           ... using undefined line width of 6.00

    WARNING: text having Multiple 0 width lines; all will be treated the same as the first.
           ... using undefined line width of 6.00



  APERTURES USED:
  ---------------------------------------------------------
  TYPE       SIZE/NAME                   ROT   MIRROR MODE 
  ---------------------------------------------------------
  CIRCLE     0.00300                                  DARK 
  CIRCLE     0.00394                                  DARK 
  CIRCLE     0.00400                                  DARK 
  CIRCLE     0.00600                                  DARK 
  CIRCLE     0.00700                                  DARK 

     BOTASSY created with warnings


================================================================
     PROCESSING FILM < LAYER2 >
     TO FILE < D:/8309 Rev.B/brd/LAYER2.art > ...
================================================================

  FILM PARAMETERS :
  ---------------------------------------------------------
  Undefined line width                6.00
  Mirror code                         NONE
  Rotate angle                        NONE
  Offset x:                           0.00
  Offset y:                           0.00
  Plot negative                       NO
  Suppress unconnected internal pads  NO



  APERTURES USED:
  ---------------------------------------------------------
  TYPE       SIZE/NAME                   ROT   MIRROR MODE 
  ---------------------------------------------------------
  CIRCLE     0.00600                                  DARK 
  CIRCLE     0.01000                                  DARK 
  CIRCLE     0.01500                                  DARK 
  CIRCLE     0.01800                                  DARK 
  CIRCLE     0.02000                                  DARK 
  CIRCLE     0.03543                                  DARK 
  CIRCLE     0.03937                                  DARK 
  CIRCLE     0.04000                                  DARK 
  CIRCLE     0.04330                                  DARK 
  CIRCLE     0.05000                                  DARK 
  CIRCLE     0.05200                                  DARK 
  CIRCLE     0.06100                                  DARK 
  CIRCLE     0.06299                                  DARK 
  CIRCLE     0.12598                                  DARK 
  CIRCLE     0.15000                                  DARK 
  OBLONG     0.06000     x 0.10800      90.000 NO     DARK 

     LAYER2 created.


================================================================
     PROCESSING FILM < LAYER3 >
     TO FILE < D:/8309 Rev.B/brd/LAYER3.art > ...
================================================================

  FILM PARAMETERS :
  ---------------------------------------------------------
  Undefined line width                6.00
  Mirror code                         NONE
  Rotate angle                        NONE
  Offset x:                           0.00
  Offset y:                           0.00
  Plot negative                       NO
  Suppress unconnected internal pads  NO



  APERTURES USED:
  ---------------------------------------------------------
  TYPE       SIZE/NAME                   ROT   MIRROR MODE 
  ---------------------------------------------------------
  CIRCLE     0.00400                                  DARK 
  CIRCLE     0.00600                                  DARK 
  CIRCLE     0.01000                                  DARK 
  CIRCLE     0.01500                                  DARK 
  CIRCLE     0.01800                                  DARK 
  CIRCLE     0.02000                                  DARK 
  CIRCLE     0.02500                                  DARK 
  CIRCLE     0.03543                                  DARK 
  CIRCLE     0.03937                                  DARK 
  CIRCLE     0.04000                                  DARK 
  CIRCLE     0.04330                                  DARK 
  CIRCLE     0.05000                                  DARK 
  CIRCLE     0.05200                                  DARK 
  CIRCLE     0.06100                                  DARK 
  CIRCLE     0.06299                                  DARK 
  CIRCLE     0.12598                                  DARK 
  CIRCLE     0.15000                                  DARK 
  OBLONG     0.06000     x 0.10800      90.000 NO     DARK 

     LAYER3 created.


================================================================
     PROCESSING FILM < LAYER4 >
     TO FILE < D:/8309 Rev.B/brd/LAYER4.art > ...
================================================================

  FILM PARAMETERS :
  ---------------------------------------------------------
  Undefined line width                6.00
  Mirror code                         NONE
  Rotate angle                        NONE
  Offset x:                           0.00
  Offset y:                           0.00
  Plot negative                       NO
  Suppress unconnected internal pads  NO



  APERTURES USED:
  ---------------------------------------------------------
  TYPE       SIZE/NAME                   ROT   MIRROR MODE 
  ---------------------------------------------------------
  CIRCLE     0.00400                                  DARK 
  CIRCLE     0.00600                                  DARK 
  CIRCLE     0.01000                                  DARK 
  CIRCLE     0.01500                                  DARK 
  CIRCLE     0.01800                                  DARK 
  CIRCLE     0.02000                                  DARK 
  CIRCLE     0.03543                                  DARK 
  CIRCLE     0.03937                                  DARK 
  CIRCLE     0.04000                                  DARK 
  CIRCLE     0.04330                                  DARK 
  CIRCLE     0.05000                                  DARK 
  CIRCLE     0.05200                                  DARK 
  CIRCLE     0.06100                                  DARK 
  CIRCLE     0.06299                                  DARK 
  CIRCLE     0.12598                                  DARK 
  CIRCLE     0.15000                                  DARK 
  OBLONG     0.06000     x 0.10800      90.000 NO     DARK 

     LAYER4 created.


================================================================
     PROCESSING FILM < BOTMASK >
     TO FILE < D:/8309 Rev.B/brd/BOTMASK.art > ...
================================================================

  FILM PARAMETERS :
  ---------------------------------------------------------
  Undefined line width                6.00
  Mirror code                         NONE
  Rotate angle                        NONE
  Offset x:                           0.00
  Offset y:                           0.00
  Plot negative                       NO
  Suppress unconnected internal pads  NO



  APERTURES USED:
  ---------------------------------------------------------
  TYPE       SIZE/NAME                   ROT   MIRROR MODE 
  ---------------------------------------------------------
  CIRCLE     0.00600                                  DARK 
  CIRCLE     0.01500                                  DARK 
  CIRCLE     0.01969                                  DARK 
  CIRCLE     0.02500                                  DARK 
  CIRCLE     0.03543                                  DARK 
  CIRCLE     0.03937                                  DARK 
  CIRCLE     0.04330                                  DARK 
  CIRCLE     0.04600                                  DARK 
  CIRCLE     0.05000                                  DARK 
  CIRCLE     0.05600                                  DARK 
  CIRCLE     0.07700                                  DARK 
  CIRCLE     0.12000                                  DARK 
  CIRCLE     0.12598                                  DARK 
  CIRCLE     0.15000                                  DARK 
  SQUARE     0.03600                     0.000 NO     DARK 
  RECTANGLE  0.01200     x 0.03400       0.000 NO     DARK 
  RECTANGLE  0.01575     x 0.01969       0.000 NO     DARK 
  RECTANGLE  0.01575     x 0.01969      90.000 NO     DARK 
  RECTANGLE  0.01600     x 0.05400      90.000 NO     DARK 
  RECTANGLE  0.01969     x 0.07874      90.000 NO     DARK 
  RECTANGLE  0.02900     x 0.02400       0.000 NO     DARK 
  RECTANGLE  0.02900     x 0.02400      90.000 NO     DARK 
  RECTANGLE  0.03000     x 0.01600       0.000 NO     DARK 
  RECTANGLE  0.03000     x 0.05000       0.000 NO     DARK 
  RECTANGLE  0.03000     x 0.05000      90.000 NO     DARK 
  RECTANGLE  0.03100     x 0.01400       0.000 NO     DARK 
  RECTANGLE  0.03100     x 0.01400      90.000 NO     DARK 
  RECTANGLE  0.03100     x 0.03500       0.000 NO     DARK 
  RECTANGLE  0.03100     x 0.03500      90.000 NO     DARK 
  RECTANGLE  0.03200     x 0.03600       0.000 NO     DARK 
  RECTANGLE  0.03200     x 0.03600      90.000 NO     DARK 
  RECTANGLE  0.03200     x 0.07500      90.000 NO     DARK 
  RECTANGLE  0.03201     x 0.17000       0.000 NO     DARK 
  RECTANGLE  0.03500     x 0.03500       0.000 NO     DARK 
  RECTANGLE  0.03500     x 0.03500      90.000 NO     DARK 
  RECTANGLE  0.03600     x 0.05600       0.000 NO     DARK 
  RECTANGLE  0.03700     x 0.04100       0.000 NO     DARK 
  RECTANGLE  0.03937     x 0.00984       0.000 NO     DARK 
  RECTANGLE  0.04100     x 0.05100       0.000 NO     DARK 
  RECTANGLE  0.04600     x 0.04100       0.000 NO     DARK 
  RECTANGLE  0.04600     x 0.04100      90.000 NO     DARK 
  RECTANGLE  0.04600     x 0.05600       0.000 NO     DARK 
  RECTANGLE  0.04600     x 0.07700      90.000 NO     DARK 
  RECTANGLE  0.05800     x 0.01500       0.000 NO     DARK 
  RECTANGLE  0.05800     x 0.01500      90.000 NO     DARK 
  RECTANGLE  0.05900     x 0.06900       0.000 NO     DARK 
  RECTANGLE  0.06502     x 0.02762       0.000 NO     DARK 
  RECTANGLE  0.06502     x 0.02762      90.000 NO     DARK 
  RECTANGLE  0.06600     x 0.11600      90.000 NO     DARK 
  RECTANGLE  0.07500     x 0.01800      90.000 NO     DARK 
  RECTANGLE  0.08400     x 0.09400       0.000 NO     DARK 
  RECTANGLE  0.08400     x 0.09400      90.000 NO     DARK 
  RECTANGLE  0.09843     x 0.18898      90.000 NO     DARK 
  RECTANGLE  0.10200     x 0.07000       0.000 NO     DARK 
  RECTANGLE  0.10500     x 0.10000       0.000 NO     DARK 
  RECTANGLE  0.10500     x 0.10000      90.000 NO     DARK 
  RECTANGLE  0.10600     x 0.18400       0.000 NO     DARK 
  OBLONG     0.06600     x 0.11400      90.000 NO     DARK 

     BOTMASK created.


================================================================
     PROCESSING FILM < BOTPASTE >
     TO FILE < D:/8309 Rev.B/brd/BOTPASTE.art > ...
================================================================

  FILM PARAMETERS :
  ---------------------------------------------------------
  Undefined line width                6.00
  Mirror code                         X
  Rotate angle                        NONE
  Offset x:                           0.00
  Offset y:                           0.00
  Plot negative                       NO
  Suppress unconnected internal pads  NO



  APERTURES USED:
  ---------------------------------------------------------
  TYPE       SIZE/NAME                   ROT   MIRROR MODE 
  ---------------------------------------------------------
  CIRCLE     0.00600                                  DARK 
  CIRCLE     0.01500                                  DARK 
  CIRCLE     0.01969                                  DARK 
  SQUARE     0.03000                     0.000 NO     DARK 
  RECTANGLE  0.01000     x 0.03200       0.000 NO     DARK 
  RECTANGLE  0.01200     x 0.05000      90.000 NO     DARK 
  RECTANGLE  0.01575     x 0.01969       0.000 NO     DARK 
  RECTANGLE  0.01575     x 0.01969      90.000 NO     DARK 
  RECTANGLE  0.01969     x 0.07874      90.000 NO     DARK 
  RECTANGLE  0.02500     x 0.02000       0.000 NO     DARK 
  RECTANGLE  0.02500     x 0.02000      90.000 NO     DARK 
  RECTANGLE  0.02700     x 0.01000       0.000 NO     DARK 
  RECTANGLE  0.02700     x 0.01000      90.000 NO     DARK 
  RECTANGLE  0.02800     x 0.01400       0.000 NO     DARK 
  RECTANGLE  0.02800     x 0.07100      90.000 NO     DARK 
  RECTANGLE  0.03000     x 0.05000       0.000 NO     DARK 
  RECTANGLE  0.03000     x 0.05000      90.000 NO     DARK 
  RECTANGLE  0.03100     x 0.03500       0.000 NO     DARK 
  RECTANGLE  0.03100     x 0.03500      90.000 NO     DARK 
  RECTANGLE  0.03200     x 0.03600       0.000 NO     DARK 
  RECTANGLE  0.03200     x 0.03600      90.000 NO     DARK 
  RECTANGLE  0.03500     x 0.03500       0.000 NO     DARK 
  RECTANGLE  0.03500     x 0.03500      90.000 NO     DARK 
  RECTANGLE  0.03500     x 0.04500       0.000 NO     DARK 
  RECTANGLE  0.03937     x 0.00984       0.000 NO     DARK 
  RECTANGLE  0.04000     x 0.03500       0.000 NO     DARK 
  RECTANGLE  0.04000     x 0.03500      90.000 NO     DARK 
  RECTANGLE  0.04000     x 0.05000       0.000 NO     DARK 
  RECTANGLE  0.04000     x 0.07100      90.000 NO     DARK 
  RECTANGLE  0.05400     x 0.01100       0.000 NO     DARK 
  RECTANGLE  0.05400     x 0.01100      90.000 NO     DARK 
  RECTANGLE  0.05500     x 0.06500       0.000 NO     DARK 
  RECTANGLE  0.06000     x 0.11000      90.000 NO     DARK 
  RECTANGLE  0.06102     x 0.02362       0.000 NO     DARK 
  RECTANGLE  0.06102     x 0.02362      90.000 NO     DARK 
  RECTANGLE  0.06500     x 0.01300      90.000 NO     DARK 
  RECTANGLE  0.08000     x 0.09000       0.000 NO     DARK 
  RECTANGLE  0.08000     x 0.09000      90.000 NO     DARK 
  RECTANGLE  0.09843     x 0.18898      90.000 NO     DARK 
  RECTANGLE  0.10000     x 0.17800       0.000 NO     DARK 
  RECTANGLE  0.10500     x 0.10000       0.000 NO     DARK 
  RECTANGLE  0.10500     x 0.10000      90.000 NO     DARK 

     BOTPASTE created.


================================================================
     PROCESSING FILM < BOTSILK >
     TO FILE < D:/8309 Rev.B/brd/BOTSILK.art > ...
================================================================

  FILM PARAMETERS :
  ---------------------------------------------------------
  Undefined line width                6.00
  Mirror code                         NONE
  Rotate angle                        NONE
  Offset x:                           0.00
  Offset y:                           0.00
  Plot negative                       NO
  Suppress unconnected internal pads  NO



  APERTURES USED:
  ---------------------------------------------------------
  TYPE       SIZE/NAME                   ROT   MIRROR MODE 
  ---------------------------------------------------------
  CIRCLE     0.00394                                  DARK 
  CIRCLE     0.00400                                  DARK 
  CIRCLE     0.00500                                  DARK 
  CIRCLE     0.00591                                  DARK 
  CIRCLE     0.00598                                  DARK 
  CIRCLE     0.00600                                  DARK 
  CIRCLE     0.00606                                  DARK 
  CIRCLE     0.00700                                  DARK 
  CIRCLE     0.00787                                  DARK 
  CIRCLE     0.00800                                  DARK 
  CIRCLE     0.00984                                  DARK 
  CIRCLE     0.01000                                  DARK 
  CIRCLE     0.01500                                  DARK 
  CIRCLE     0.02362                                  DARK 

     BOTSILK created.


================================================================
     PROCESSING FILM < BOTTOM >
     TO FILE < D:/8309 Rev.B/brd/BOTTOM.art > ...
================================================================

  FILM PARAMETERS :
  ---------------------------------------------------------
  Undefined line width                6.00
  Mirror code                         NONE
  Rotate angle                        NONE
  Offset x:                           0.00
  Offset y:                           0.00
  Plot negative                       NO
  Suppress unconnected internal pads  NO



  APERTURES USED:
  ---------------------------------------------------------
  TYPE       SIZE/NAME                   ROT   MIRROR MODE 
  ---------------------------------------------------------
  CIRCLE     0.00400                                  DARK 
  CIRCLE     0.00600                                  DARK 
  CIRCLE     0.01000                                  DARK 
  CIRCLE     0.01200                                  DARK 
  CIRCLE     0.01500                                  DARK 
  CIRCLE     0.01600                                  DARK 
  CIRCLE     0.01800                                  DARK 
  CIRCLE     0.01969                                  DARK 
  CIRCLE     0.02000                                  DARK 
  CIRCLE     0.02500                                  DARK 
  CIRCLE     0.03000                                  DARK 
  CIRCLE     0.03543                                  DARK 
  CIRCLE     0.03937                                  DARK 
  CIRCLE     0.04000                                  DARK 
  CIRCLE     0.04330                                  DARK 
  CIRCLE     0.05000                                  DARK 
  CIRCLE     0.05200                                  DARK 
  CIRCLE     0.06100                                  DARK 
  CIRCLE     0.06299                                  DARK 
  CIRCLE     0.12598                                  DARK 
  CIRCLE     0.15000                                  DARK 
  SQUARE     0.03000                     0.000 NO     DARK 
  RECTANGLE  0.01000     x 0.03200       0.000 NO     DARK 
  RECTANGLE  0.01200     x 0.05000      90.000 NO     DARK 
  RECTANGLE  0.01575     x 0.01969       0.000 NO     DARK 
  RECTANGLE  0.01575     x 0.01969      90.000 NO     DARK 
  RECTANGLE  0.01969     x 0.07874      90.000 NO     DARK 
  RECTANGLE  0.02500     x 0.02000       0.000 NO     DARK 
  RECTANGLE  0.02500     x 0.02000      90.000 NO     DARK 
  RECTANGLE  0.02700     x 0.01000       0.000 NO     DARK 
  RECTANGLE  0.02700     x 0.01000      90.000 NO     DARK 
  RECTANGLE  0.02799     x 0.16598       0.000 NO     DARK 
  RECTANGLE  0.02800     x 0.07100      90.000 NO     DARK 
  RECTANGLE  0.03000     x 0.01600       0.000 NO     DARK 
  RECTANGLE  0.03000     x 0.05000       0.000 NO     DARK 
  RECTANGLE  0.03000     x 0.05000      90.000 NO     DARK 
  RECTANGLE  0.03100     x 0.03500       0.000 NO     DARK 
  RECTANGLE  0.03100     x 0.03500      90.000 NO     DARK 
  RECTANGLE  0.03200     x 0.03600       0.000 NO     DARK 
  RECTANGLE  0.03200     x 0.03600      90.000 NO     DARK 
  RECTANGLE  0.03500     x 0.03500       0.000 NO     DARK 
  RECTANGLE  0.03500     x 0.03500      90.000 NO     DARK 
  RECTANGLE  0.03500     x 0.04500       0.000 NO     DARK 
  RECTANGLE  0.03937     x 0.00984       0.000 NO     DARK 
  RECTANGLE  0.04000     x 0.03500       0.000 NO     DARK 
  RECTANGLE  0.04000     x 0.03500      90.000 NO     DARK 
  RECTANGLE  0.04000     x 0.05000       0.000 NO     DARK 
  RECTANGLE  0.04000     x 0.07100      90.000 NO     DARK 
  RECTANGLE  0.05400     x 0.01100       0.000 NO     DARK 
  RECTANGLE  0.05400     x 0.01100      90.000 NO     DARK 
  RECTANGLE  0.05500     x 0.06500       0.000 NO     DARK 
  RECTANGLE  0.06000     x 0.11000      90.000 NO     DARK 
  RECTANGLE  0.06102     x 0.02362       0.000 NO     DARK 
  RECTANGLE  0.06102     x 0.02362      90.000 NO     DARK 
  RECTANGLE  0.06500     x 0.01300      90.000 NO     DARK 
  RECTANGLE  0.08000     x 0.09000       0.000 NO     DARK 
  RECTANGLE  0.08000     x 0.09000      90.000 NO     DARK 
  RECTANGLE  0.09800     x 0.06600       0.000 NO     DARK 
  RECTANGLE  0.09843     x 0.18898      90.000 NO     DARK 
  RECTANGLE  0.10000     x 0.17800       0.000 NO     DARK 
  RECTANGLE  0.10500     x 0.10000       0.000 NO     DARK 
  RECTANGLE  0.10500     x 0.10000      90.000 NO     DARK 
  OBLONG     0.06000     x 0.10800      90.000 NO     DARK 

     BOTTOM created.


================================================================
     PROCESSING FILM < LAYER5 >
     TO FILE < D:/8309 Rev.B/brd/LAYER5.art > ...
================================================================

  FILM PARAMETERS :
  ---------------------------------------------------------
  Undefined line width                6.00
  Mirror code                         NONE
  Rotate angle                        NONE
  Offset x:                           0.00
  Offset y:                           0.00
  Plot negative                       NO
  Suppress unconnected internal pads  NO



  APERTURES USED:
  ---------------------------------------------------------
  TYPE       SIZE/NAME                   ROT   MIRROR MODE 
  ---------------------------------------------------------
  CIRCLE     0.00600                                  DARK 
  CIRCLE     0.01000                                  DARK 
  CIRCLE     0.01500                                  DARK 
  CIRCLE     0.01800                                  DARK 
  CIRCLE     0.02000                                  DARK 
  CIRCLE     0.03543                                  DARK 
  CIRCLE     0.03937                                  DARK 
  CIRCLE     0.04000                                  DARK 
  CIRCLE     0.04330                                  DARK 
  CIRCLE     0.05000                                  DARK 
  CIRCLE     0.05200                                  DARK 
  CIRCLE     0.06100                                  DARK 
  CIRCLE     0.06299                                  DARK 
  CIRCLE     0.12598                                  DARK 
  CIRCLE     0.15000                                  DARK 
  OBLONG     0.06000     x 0.10800      90.000 NO     DARK 

     LAYER5 created.


================================================================
     PROCESSING FILM < TOP >
     TO FILE < D:/8309 Rev.B/brd/TOP.art > ...
================================================================

  FILM PARAMETERS :
  ---------------------------------------------------------
  Undefined line width                6.00
  Mirror code                         NONE
  Rotate angle                        NONE
  Offset x:                           0.00
  Offset y:                           0.00
  Plot negative                       NO
  Suppress unconnected internal pads  NO



  APERTURES USED:
  ---------------------------------------------------------
  TYPE       SIZE/NAME                   ROT   MIRROR MODE 
  ---------------------------------------------------------
  CIRCLE     0.00400                                  DARK 
  CIRCLE     0.00600                                  DARK 
  CIRCLE     0.01000                                  DARK 
  CIRCLE     0.01500                                  DARK 
  CIRCLE     0.01600                                  DARK 
  CIRCLE     0.01800                                  DARK 
  CIRCLE     0.01969                                  DARK 
  CIRCLE     0.02000                                  DARK 
  CIRCLE     0.03000                                  DARK 
  CIRCLE     0.03543                                  DARK 
  CIRCLE     0.03937                                  DARK 
  CIRCLE     0.04000                                  DARK 
  CIRCLE     0.04330                                  DARK 
  CIRCLE     0.05000                                  DARK 
  CIRCLE     0.05200                                  DARK 
  CIRCLE     0.06100                                  DARK 
  CIRCLE     0.06299                                  DARK 
  CIRCLE     0.12598                                  DARK 
  CIRCLE     0.15000                                  DARK 
  SQUARE     0.03000                     0.000 NO     DARK 
  SQUARE     0.14000                     0.000 NO     DARK 
  RECTANGLE  0.01200     x 0.04000       0.000 NO     DARK 
  RECTANGLE  0.01200     x 0.04000      90.000 NO     DARK 
  RECTANGLE  0.01200     x 0.05000      90.000 NO     DARK 
  RECTANGLE  0.01575     x 0.01969       0.000 NO     DARK 
  RECTANGLE  0.01575     x 0.01969      90.000 NO     DARK 
  RECTANGLE  0.01969     x 0.09055      90.000 NO     DARK 
  RECTANGLE  0.02000     x 0.09055      90.000 NO     DARK 
  RECTANGLE  0.02500     x 0.02000       0.000 NO     DARK 
  RECTANGLE  0.02799     x 0.16598       0.000 NO     DARK 
  RECTANGLE  0.02800     x 0.01200       0.000 NO     DARK 
  RECTANGLE  0.03000     x 0.05000       0.000 NO     DARK 
  RECTANGLE  0.03100     x 0.03500      90.000 NO     DARK 
  RECTANGLE  0.03200     x 0.03600       0.000 NO     DARK 
  RECTANGLE  0.03200     x 0.03600      90.000 NO     DARK 
  RECTANGLE  0.03500     x 0.03500       0.000 NO     DARK 
  RECTANGLE  0.03500     x 0.03500      90.000 NO     DARK 
  RECTANGLE  0.03500     x 0.04500       0.000 NO     DARK 
  RECTANGLE  0.03600     x 0.04800       0.000 NO     DARK 
  RECTANGLE  0.03600     x 0.04800      90.000 NO     DARK 
  RECTANGLE  0.04000     x 0.03500       0.000 NO     DARK 
  RECTANGLE  0.04000     x 0.03500      90.000 NO     DARK 
  RECTANGLE  0.04000     x 0.05000       0.000 NO     DARK 
  RECTANGLE  0.04400     x 0.03200      90.000 NO     DARK 
  RECTANGLE  0.04400     x 0.07200      90.000 NO     DARK 
  RECTANGLE  0.05000     x 0.03000       0.000 NO     DARK 
  RECTANGLE  0.05000     x 0.10000      90.000 NO     DARK 
  RECTANGLE  0.05000     x 0.12500      90.000 NO     DARK 
  RECTANGLE  0.05906     x 0.07874      90.000 NO     DARK 
  RECTANGLE  0.06000     x 0.01800       0.000 NO     DARK 
  RECTANGLE  0.06102     x 0.02362       0.000 NO     DARK 
  RECTANGLE  0.06500     x 0.01300       0.000 NO     DARK 
  RECTANGLE  0.06500     x 0.01300      90.000 NO     DARK 
  RECTANGLE  0.07100     x 0.07900      90.000 NO     DARK 
  RECTANGLE  0.07874     x 0.09900      90.000 NO     DARK 
  RECTANGLE  0.08000     x 0.09000       0.000 NO     DARK 
  RECTANGLE  0.08000     x 0.09000      90.000 NO     DARK 
  RECTANGLE  0.08000     x 0.14000      90.000 NO     DARK 
  RECTANGLE  0.09500     x 0.10500       0.000 NO     DARK 
  RECTANGLE  0.09500     x 0.12000       0.000 NO     DARK 
  RECTANGLE  0.10000     x 0.02800      90.000 NO     DARK 
  RECTANGLE  0.12000     x 0.10000       0.000 NO     DARK 
  RECTANGLE  0.25000     x 0.05000      90.000 NO     DARK 
  OBLONG     0.06000     x 0.10800      90.000 NO     DARK 

     TOP created.


================================================================
     PROCESSING FILM < TOPASSY >
     TO FILE < D:/8309 Rev.B/brd/TOPASSY.art > ...
================================================================

  FILM PARAMETERS :
  ---------------------------------------------------------
  Undefined line width                6.00
  Mirror code                         NONE
  Rotate angle                        NONE
  Offset x:                           0.00
  Offset y:                           0.00
  Plot negative                       NO
  Suppress unconnected internal pads  NO



  APERTURES USED:
  ---------------------------------------------------------
  TYPE       SIZE/NAME                   ROT   MIRROR MODE 
  ---------------------------------------------------------
  CIRCLE     0.00394                                  DARK 
  CIRCLE     0.00400                                  DARK 
  CIRCLE     0.00591                                  DARK 
  CIRCLE     0.00598                                  DARK 
  CIRCLE     0.00600                                  DARK 
  CIRCLE     0.00606                                  DARK 
  CIRCLE     0.00700                                  DARK 

     TOPASSY created.


================================================================
     PROCESSING FILM < TOPMASK >
     TO FILE < D:/8309 Rev.B/brd/TOPMASK.art > ...
================================================================

  FILM PARAMETERS :
  ---------------------------------------------------------
  Undefined line width                6.00
  Mirror code                         NONE
  Rotate angle                        NONE
  Offset x:                           0.00
  Offset y:                           0.00
  Plot negative                       NO
  Suppress unconnected internal pads  NO



  APERTURES USED:
  ---------------------------------------------------------
  TYPE       SIZE/NAME                   ROT   MIRROR MODE 
  ---------------------------------------------------------
  CIRCLE     0.00600                                  DARK 
  CIRCLE     0.01500                                  DARK 
  CIRCLE     0.01600                                  DARK 
  CIRCLE     0.01800                                  DARK 
  CIRCLE     0.01969                                  DARK 
  CIRCLE     0.02100                                  DARK 
  CIRCLE     0.03543                                  DARK 
  CIRCLE     0.03937                                  DARK 
  CIRCLE     0.04330                                  DARK 
  CIRCLE     0.04600                                  DARK 
  CIRCLE     0.05000                                  DARK 
  CIRCLE     0.05600                                  DARK 
  CIRCLE     0.07700                                  DARK 
  CIRCLE     0.12000                                  DARK 
  CIRCLE     0.12598                                  DARK 
  CIRCLE     0.15000                                  DARK 
  SQUARE     0.03600                     0.000 NO     DARK 
  SQUARE     0.15000                     0.000 NO     DARK 
  RECTANGLE  0.01575     x 0.01969       0.000 NO     DARK 
  RECTANGLE  0.01575     x 0.01969      90.000 NO     DARK 
  RECTANGLE  0.01600     x 0.05400      90.000 NO     DARK 
  RECTANGLE  0.01700     x 0.04500       0.000 NO     DARK 
  RECTANGLE  0.01700     x 0.04500      90.000 NO     DARK 
  RECTANGLE  0.01969     x 0.09055      90.000 NO     DARK 
  RECTANGLE  0.02400     x 0.09455      90.000 NO     DARK 
  RECTANGLE  0.02900     x 0.02400       0.000 NO     DARK 
  RECTANGLE  0.03100     x 0.03500      90.000 NO     DARK 
  RECTANGLE  0.03200     x 0.01600       0.000 NO     DARK 
  RECTANGLE  0.03200     x 0.03600       0.000 NO     DARK 
  RECTANGLE  0.03200     x 0.03600      90.000 NO     DARK 
  RECTANGLE  0.03201     x 0.17000       0.000 NO     DARK 
  RECTANGLE  0.03500     x 0.03500       0.000 NO     DARK 
  RECTANGLE  0.03500     x 0.03500      90.000 NO     DARK 
  RECTANGLE  0.03600     x 0.05600       0.000 NO     DARK 
  RECTANGLE  0.04000     x 0.05200       0.000 NO     DARK 
  RECTANGLE  0.04000     x 0.05200      90.000 NO     DARK 
  RECTANGLE  0.04100     x 0.05100       0.000 NO     DARK 
  RECTANGLE  0.04400     x 0.03200      90.000 NO     DARK 
  RECTANGLE  0.04400     x 0.07200      90.000 NO     DARK 
  RECTANGLE  0.04600     x 0.04100       0.000 NO     DARK 
  RECTANGLE  0.04600     x 0.04100      90.000 NO     DARK 
  RECTANGLE  0.04600     x 0.05600       0.000 NO     DARK 
  RECTANGLE  0.05000     x 0.03000       0.000 NO     DARK 
  RECTANGLE  0.05400     x 0.10400      90.000 NO     DARK 
  RECTANGLE  0.05400     x 0.12900      90.000 NO     DARK 
  RECTANGLE  0.05906     x 0.07874      90.000 NO     DARK 
  RECTANGLE  0.06000     x 0.01800       0.000 NO     DARK 
  RECTANGLE  0.06502     x 0.02762       0.000 NO     DARK 
  RECTANGLE  0.07100     x 0.07900      90.000 NO     DARK 
  RECTANGLE  0.07500     x 0.01800       0.000 NO     DARK 
  RECTANGLE  0.07500     x 0.01800      90.000 NO     DARK 
  RECTANGLE  0.07874     x 0.09900      90.000 NO     DARK 
  RECTANGLE  0.08400     x 0.09400       0.000 NO     DARK 
  RECTANGLE  0.08400     x 0.09400      90.000 NO     DARK 
  RECTANGLE  0.08500     x 0.14500      90.000 NO     DARK 
  RECTANGLE  0.09500     x 0.10500       0.000 NO     DARK 
  RECTANGLE  0.09500     x 0.12000       0.000 NO     DARK 
  RECTANGLE  0.10400     x 0.03200      90.000 NO     DARK 
  RECTANGLE  0.12500     x 0.10500       0.000 NO     DARK 
  RECTANGLE  0.25500     x 0.05500      90.000 NO     DARK 
  OBLONG     0.06600     x 0.11400      90.000 NO     DARK 

     TOPMASK created.


================================================================
     PROCESSING FILM < TOPPASTE >
     TO FILE < D:/8309 Rev.B/brd/TOPPASTE.art > ...
================================================================

  FILM PARAMETERS :
  ---------------------------------------------------------
  Undefined line width                6.00
  Mirror code                         NONE
  Rotate angle                        NONE
  Offset x:                           0.00
  Offset y:                           0.00
  Plot negative                       NO
  Suppress unconnected internal pads  NO



  APERTURES USED:
  ---------------------------------------------------------
  TYPE       SIZE/NAME                   ROT   MIRROR MODE 
  ---------------------------------------------------------
  CIRCLE     0.00600                                  DARK 
  CIRCLE     0.01500                                  DARK 
  CIRCLE     0.01600                                  DARK 
  CIRCLE     0.01800                                  DARK 
  CIRCLE     0.01969                                  DARK 
  SQUARE     0.03000                     0.000 NO     DARK 
  SQUARE     0.05906                     0.000 NO     DARK 
  RECTANGLE  0.01200     x 0.04000       0.000 NO     DARK 
  RECTANGLE  0.01200     x 0.04000      90.000 NO     DARK 
  RECTANGLE  0.01200     x 0.05000      90.000 NO     DARK 
  RECTANGLE  0.01575     x 0.01969       0.000 NO     DARK 
  RECTANGLE  0.01575     x 0.01969      90.000 NO     DARK 
  RECTANGLE  0.01969     x 0.09055      90.000 NO     DARK 
  RECTANGLE  0.02000     x 0.09055      90.000 NO     DARK 
  RECTANGLE  0.02500     x 0.02000       0.000 NO     DARK 
  RECTANGLE  0.02800     x 0.01200       0.000 NO     DARK 
  RECTANGLE  0.03000     x 0.05000       0.000 NO     DARK 
  RECTANGLE  0.03100     x 0.03500      90.000 NO     DARK 
  RECTANGLE  0.03200     x 0.03600       0.000 NO     DARK 
  RECTANGLE  0.03200     x 0.03600      90.000 NO     DARK 
  RECTANGLE  0.03500     x 0.03500       0.000 NO     DARK 
  RECTANGLE  0.03500     x 0.03500      90.000 NO     DARK 
  RECTANGLE  0.03500     x 0.04500       0.000 NO     DARK 
  RECTANGLE  0.03600     x 0.04800       0.000 NO     DARK 
  RECTANGLE  0.03600     x 0.04800      90.000 NO     DARK 
  RECTANGLE  0.04000     x 0.03500       0.000 NO     DARK 
  RECTANGLE  0.04000     x 0.03500      90.000 NO     DARK 
  RECTANGLE  0.04000     x 0.05000       0.000 NO     DARK 
  RECTANGLE  0.04400     x 0.03200      90.000 NO     DARK 
  RECTANGLE  0.04400     x 0.07200      90.000 NO     DARK 
  RECTANGLE  0.04800     x 0.09800      90.000 NO     DARK 
  RECTANGLE  0.05000     x 0.03000       0.000 NO     DARK 
  RECTANGLE  0.05000     x 0.12500      90.000 NO     DARK 
  RECTANGLE  0.05500     x 0.01600       0.000 NO     DARK 
  RECTANGLE  0.06102     x 0.02362       0.000 NO     DARK 
  RECTANGLE  0.06500     x 0.01300       0.000 NO     DARK 
  RECTANGLE  0.06500     x 0.01300      90.000 NO     DARK 
  RECTANGLE  0.07100     x 0.07900      90.000 NO     DARK 
  RECTANGLE  0.07874     x 0.09900      90.000 NO     DARK 
  RECTANGLE  0.08000     x 0.09000       0.000 NO     DARK 
  RECTANGLE  0.08000     x 0.09000      90.000 NO     DARK 
  RECTANGLE  0.08000     x 0.14000      90.000 NO     DARK 
  RECTANGLE  0.09500     x 0.10500       0.000 NO     DARK 
  RECTANGLE  0.09500     x 0.12000       0.000 NO     DARK 
  RECTANGLE  0.10000     x 0.02800      90.000 NO     DARK 
  RECTANGLE  0.12000     x 0.10000       0.000 NO     DARK 
  RECTANGLE  0.25000     x 0.05000      90.000 NO     DARK 

     TOPPASTE created.


================================================================
     PROCESSING FILM < TOPSILK >
     TO FILE < D:/8309 Rev.B/brd/TOPSILK.art > ...
================================================================

  FILM PARAMETERS :
  ---------------------------------------------------------
  Undefined line width                6.00
  Mirror code                         NONE
  Rotate angle                        NONE
  Offset x:                           0.00
  Offset y:                           0.00
  Plot negative                       NO
  Suppress unconnected internal pads  NO



  APERTURES USED:
  ---------------------------------------------------------
  TYPE       SIZE/NAME                   ROT   MIRROR MODE 
  ---------------------------------------------------------
  CIRCLE     0.00394                                  DARK 
  CIRCLE     0.00400                                  DARK 
  CIRCLE     0.00500                                  DARK 
  CIRCLE     0.00591                                  DARK 
  CIRCLE     0.00598                                  DARK 
  CIRCLE     0.00600                                  DARK 
  CIRCLE     0.00700                                  DARK 
  CIRCLE     0.00787                                  DARK 
  CIRCLE     0.00800                                  DARK 
  CIRCLE     0.00984                                  DARK 
  CIRCLE     0.01000                                  DARK 
  CIRCLE     0.01500                                  DARK 
  CIRCLE     0.02362                                  DARK 

     TOPSILK created.


================================================================
     PROCESSING FILM < FABRICATION >
     TO FILE < D:/8309 Rev.B/brd/FABRICATION.art > ...
================================================================

  FILM PARAMETERS :
  ---------------------------------------------------------
  Undefined line width                6.00
  Mirror code                         NONE
  Rotate angle                        NONE
  Offset x:                           0.00
  Offset y:                           0.00
  Plot negative                       NO
  Suppress unconnected internal pads  NO



  APERTURES USED:
  ---------------------------------------------------------
  TYPE       SIZE/NAME                   ROT   MIRROR MODE 
  ---------------------------------------------------------
  CIRCLE     0.00600                                  DARK 

     FABRICATION created.


================================================================
     PROCESSING FILM < TOP_PLACE >
     TO FILE < D:/8309 Rev.B/brd/TOP_PLACE.art > ...
================================================================

  FILM PARAMETERS :
  ---------------------------------------------------------
  Undefined line width                0.00
  Mirror code                         NONE
  Rotate angle                        NONE
  Offset x:                           0.00
  Offset y:                           0.00
  Plot negative                       NO
  Suppress unconnected internal pads  NO

    WARNING: rectangle or unfilled shape composed 0 width line found at (1722.46 1870.46)
           ... ignored!

    WARNING: rectangle or unfilled shape having Multiple 0 width lines; all will be treated the same as the first.
           ... ignored!



  APERTURES USED:
  ---------------------------------------------------------
  TYPE       SIZE/NAME                   ROT   MIRROR MODE 
  ---------------------------------------------------------
  CIRCLE     0.00394                                  DARK 
  CIRCLE     0.00400                                  DARK 
  CIRCLE     0.00500                                  DARK 
  CIRCLE     0.00591                                  DARK 
  CIRCLE     0.00598                                  DARK 
  CIRCLE     0.00600                                  DARK 
  CIRCLE     0.00700                                  DARK 
  CIRCLE     0.00787                                  DARK 
  CIRCLE     0.00800                                  DARK 
  CIRCLE     0.00984                                  DARK 
  CIRCLE     0.01000                                  DARK 
  CIRCLE     0.01500                                  DARK 
  CIRCLE     0.01600                                  DARK 
  CIRCLE     0.01800                                  DARK 
  CIRCLE     0.01969                                  DARK 
  CIRCLE     0.02000                                  DARK 
  CIRCLE     0.02362                                  DARK 
  CIRCLE     0.03000                                  DARK 
  CIRCLE     0.03543                                  DARK 
  CIRCLE     0.03937                                  DARK 
  CIRCLE     0.04000                                  DARK 
  CIRCLE     0.04330                                  DARK 
  CIRCLE     0.05000                                  DARK 
  CIRCLE     0.05200                                  DARK 
  CIRCLE     0.06100                                  DARK 
  CIRCLE     0.06299                                  DARK 
  CIRCLE     0.12598                                  DARK 
  CIRCLE     0.15000                                  DARK 
  SQUARE     0.03000                     0.000 NO     DARK 
  SQUARE     0.14000                     0.000 NO     DARK 
  RECTANGLE  0.01200     x 0.04000       0.000 NO     DARK 
  RECTANGLE  0.01200     x 0.04000      90.000 NO     DARK 
  RECTANGLE  0.01200     x 0.05000      90.000 NO     DARK 
  RECTANGLE  0.01575     x 0.01969       0.000 NO     DARK 
  RECTANGLE  0.01575     x 0.01969      90.000 NO     DARK 
  RECTANGLE  0.01969     x 0.09055      90.000 NO     DARK 
  RECTANGLE  0.02000     x 0.09055      90.000 NO     DARK 
  RECTANGLE  0.02500     x 0.02000       0.000 NO     DARK 
  RECTANGLE  0.02799     x 0.16598       0.000 NO     DARK 
  RECTANGLE  0.02800     x 0.01200       0.000 NO     DARK 
  RECTANGLE  0.03000     x 0.05000       0.000 NO     DARK 
  RECTANGLE  0.03100     x 0.03500      90.000 NO     DARK 
  RECTANGLE  0.03200     x 0.03600       0.000 NO     DARK 
  RECTANGLE  0.03200     x 0.03600      90.000 NO     DARK 
  RECTANGLE  0.03500     x 0.03500       0.000 NO     DARK 
  RECTANGLE  0.03500     x 0.03500      90.000 NO     DARK 
  RECTANGLE  0.03500     x 0.04500       0.000 NO     DARK 
  RECTANGLE  0.03600     x 0.04800       0.000 NO     DARK 
  RECTANGLE  0.03600     x 0.04800      90.000 NO     DARK 
  RECTANGLE  0.04000     x 0.03500       0.000 NO     DARK 
  RECTANGLE  0.04000     x 0.03500      90.000 NO     DARK 
  RECTANGLE  0.04000     x 0.05000       0.000 NO     DARK 
  RECTANGLE  0.04400     x 0.03200      90.000 NO     DARK 
  RECTANGLE  0.04400     x 0.07200      90.000 NO     DARK 
  RECTANGLE  0.05000     x 0.03000       0.000 NO     DARK 
  RECTANGLE  0.05000     x 0.10000      90.000 NO     DARK 
  RECTANGLE  0.05000     x 0.12500      90.000 NO     DARK 
  RECTANGLE  0.05906     x 0.07874      90.000 NO     DARK 
  RECTANGLE  0.06000     x 0.01800       0.000 NO     DARK 
  RECTANGLE  0.06102     x 0.02362       0.000 NO     DARK 
  RECTANGLE  0.06500     x 0.01300       0.000 NO     DARK 
  RECTANGLE  0.06500     x 0.01300      90.000 NO     DARK 
  RECTANGLE  0.07100     x 0.07900      90.000 NO     DARK 
  RECTANGLE  0.07874     x 0.09900      90.000 NO     DARK 
  RECTANGLE  0.08000     x 0.09000       0.000 NO     DARK 
  RECTANGLE  0.08000     x 0.09000      90.000 NO     DARK 
  RECTANGLE  0.08000     x 0.14000      90.000 NO     DARK 
  RECTANGLE  0.09500     x 0.10500       0.000 NO     DARK 
  RECTANGLE  0.09500     x 0.12000       0.000 NO     DARK 
  RECTANGLE  0.10000     x 0.02800      90.000 NO     DARK 
  RECTANGLE  0.12000     x 0.10000       0.000 NO     DARK 
  RECTANGLE  0.25000     x 0.05000      90.000 NO     DARK 
  OBLONG     0.06000     x 0.10800      90.000 NO     DARK 

     TOP_PLACE created with warnings


================================================================
     PROCESSING FILM < BOT_PLACE >
     TO FILE < D:/8309 Rev.B/brd/BOT_PLACE.art > ...
================================================================

  FILM PARAMETERS :
  ---------------------------------------------------------
  Undefined line width                0.00
  Mirror code                         NONE
  Rotate angle                        NONE
  Offset x:                           0.00
  Offset y:                           0.00
  Plot negative                       NO
  Suppress unconnected internal pads  NO


    ERROR: aborting film - Shape with first seg=(1696.46 1336.46) [layer=BOTTOM]
	has a void with extents [(1814.39 1650.44) (1934.43 1722.48)] that touches
	another shape with first seg=(1171.46 -673.54). Manually resolve problem.

    ERROR: aborting film - artwork will not be generated!
 Error in BOT_PLACE--halting output.  Artwork file not generated.
 *** ERROR with BOT_PLACE




================================================================
     PROCESSING FILM < TOP_ROUTE >
     TO FILE < D:/8309 Rev.B/brd/TOP_ROUTE.art > ...
================================================================

  FILM PARAMETERS :
  ---------------------------------------------------------
  Undefined line width                0.00
  Mirror code                         NONE
  Rotate angle                        NONE
  Offset x:                           0.00
  Offset y:                           0.00
  Plot negative                       NO
  Suppress unconnected internal pads  NO



  APERTURES USED:
  ---------------------------------------------------------
  TYPE       SIZE/NAME                   ROT   MIRROR MODE 
  ---------------------------------------------------------
  CIRCLE     0.00394                                  DARK 
  CIRCLE     0.00400                                  DARK 
  CIRCLE     0.00500                                  DARK 
  CIRCLE     0.00591                                  DARK 
  CIRCLE     0.00598                                  DARK 
  CIRCLE     0.00600                                  DARK 
  CIRCLE     0.00700                                  DARK 
  CIRCLE     0.00787                                  DARK 
  CIRCLE     0.00800                                  DARK 
  CIRCLE     0.00984                                  DARK 
  CIRCLE     0.01000                                  DARK 
  CIRCLE     0.01500                                  DARK 
  CIRCLE     0.01600                                  DARK 
  CIRCLE     0.01800                                  DARK 
  CIRCLE     0.01969                                  DARK 
  CIRCLE     0.02000                                  DARK 
  CIRCLE     0.02362                                  DARK 
  CIRCLE     0.03000                                  DARK 
  CIRCLE     0.03543                                  DARK 
  CIRCLE     0.03937                                  DARK 
  CIRCLE     0.04000                                  DARK 
  CIRCLE     0.04330                                  DARK 
  CIRCLE     0.05000                                  DARK 
  CIRCLE     0.05200                                  DARK 
  CIRCLE     0.06100                                  DARK 
  CIRCLE     0.06299                                  DARK 
  CIRCLE     0.12598                                  DARK 
  CIRCLE     0.15000                                  DARK 
  SQUARE     0.03000                     0.000 NO     DARK 
  SQUARE     0.14000                     0.000 NO     DARK 
  RECTANGLE  0.01200     x 0.04000       0.000 NO     DARK 
  RECTANGLE  0.01200     x 0.04000      90.000 NO     DARK 
  RECTANGLE  0.01200     x 0.05000      90.000 NO     DARK 
  RECTANGLE  0.01575     x 0.01969       0.000 NO     DARK 
  RECTANGLE  0.01575     x 0.01969      90.000 NO     DARK 
  RECTANGLE  0.01969     x 0.09055      90.000 NO     DARK 
  RECTANGLE  0.02000     x 0.09055      90.000 NO     DARK 
  RECTANGLE  0.02500     x 0.02000       0.000 NO     DARK 
  RECTANGLE  0.02799     x 0.16598       0.000 NO     DARK 
  RECTANGLE  0.02800     x 0.01200       0.000 NO     DARK 
  RECTANGLE  0.03000     x 0.05000       0.000 NO     DARK 
  RECTANGLE  0.03100     x 0.03500      90.000 NO     DARK 
  RECTANGLE  0.03200     x 0.03600       0.000 NO     DARK 
  RECTANGLE  0.03200     x 0.03600      90.000 NO     DARK 
  RECTANGLE  0.03500     x 0.03500       0.000 NO     DARK 
  RECTANGLE  0.03500     x 0.03500      90.000 NO     DARK 
  RECTANGLE  0.03500     x 0.04500       0.000 NO     DARK 
  RECTANGLE  0.03600     x 0.04800       0.000 NO     DARK 
  RECTANGLE  0.03600     x 0.04800      90.000 NO     DARK 
  RECTANGLE  0.04000     x 0.03500       0.000 NO     DARK 
  RECTANGLE  0.04000     x 0.03500      90.000 NO     DARK 
  RECTANGLE  0.04000     x 0.05000       0.000 NO     DARK 
  RECTANGLE  0.04400     x 0.03200      90.000 NO     DARK 
  RECTANGLE  0.04400     x 0.07200      90.000 NO     DARK 
  RECTANGLE  0.05000     x 0.03000       0.000 NO     DARK 
  RECTANGLE  0.05000     x 0.10000      90.000 NO     DARK 
  RECTANGLE  0.05000     x 0.12500      90.000 NO     DARK 
  RECTANGLE  0.05906     x 0.07874      90.000 NO     DARK 
  RECTANGLE  0.06000     x 0.01800       0.000 NO     DARK 
  RECTANGLE  0.06102     x 0.02362       0.000 NO     DARK 
  RECTANGLE  0.06500     x 0.01300       0.000 NO     DARK 
  RECTANGLE  0.06500     x 0.01300      90.000 NO     DARK 
  RECTANGLE  0.07100     x 0.07900      90.000 NO     DARK 
  RECTANGLE  0.07874     x 0.09900      90.000 NO     DARK 
  RECTANGLE  0.08000     x 0.09000       0.000 NO     DARK 
  RECTANGLE  0.08000     x 0.09000      90.000 NO     DARK 
  RECTANGLE  0.08000     x 0.14000      90.000 NO     DARK 
  RECTANGLE  0.09500     x 0.10500       0.000 NO     DARK 
  RECTANGLE  0.09500     x 0.12000       0.000 NO     DARK 
  RECTANGLE  0.10000     x 0.02800      90.000 NO     DARK 
  RECTANGLE  0.12000     x 0.10000       0.000 NO     DARK 
  RECTANGLE  0.25000     x 0.05000      90.000 NO     DARK 
  OBLONG     0.06000     x 0.10800      90.000 NO     DARK 

     TOP_ROUTE created.


================================================================
     PROCESSING FILM < PLACEMENT >
     TO FILE < D:/8309 Rev.B/brd/PLACEMENT.art > ...
================================================================

  FILM PARAMETERS :
  ---------------------------------------------------------
  Undefined line width                0.00
  Mirror code                         NONE
  Rotate angle                        NONE
  Offset x:                           0.00
  Offset y:                           0.00
  Plot negative                       NO
  Suppress unconnected internal pads  NO

    WARNING: more than one pin class in film record
    WARNING: more than one via class in film record
    WARNING: more than one etch class in film record
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_40_GFU at (-2173.54 -598.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_40_GFU at (-2173.54 -598.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_40_GFU at (-2173.54 1781.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_40_GFU at (-2173.54 1781.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_79_99 at (-1969.68 661.26).
    WARNING: Null REGULAR-PAD specified for padstack RECT60X110 at (-1992.41 738.43).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_79_99 at (-1969.68 1011.66).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_59_79 at (-2019.84 1112.40).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_59_79 at (-2019.84 1230.52).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_59_79 at (-2019.84 1372.40).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_59_79 at (-2019.84 1490.52).
    WARNING: Null REGULAR-PAD specified for padstack RECT60X110 at (-1992.41 1813.24).
    WARNING: Null REGULAR-PAD specified for padstack SMD40_35 at (-1723.54 616.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_91 at (-1749.15 836.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_91 at (-1749.15 804.96).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_91 at (-1749.15 773.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_79_99 at (-1753.15 661.26).
    WARNING: Null REGULAR-PAD specified for padstack SMD40_35 at (-1723.54 676.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_91 at (-1749.15 899.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_91 at (-1749.15 867.96).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_79_99 at (-1753.15 1011.66).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_59_79 at (-1807.24 1230.52).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_59_79 at (-1807.24 1112.40).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_59_79 at (-1807.24 1372.40).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1788.85 1301.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1828.23 1301.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_59_79 at (-1807.24 1490.52).
    WARNING: Null REGULAR-PAD specified for padstack PAD50X100 at (-1831.06 1601.46).
    WARNING: Null REGULAR-PAD specified for padstack PAD50X100 at (-1831.06 1701.46).
    WARNING: Null REGULAR-PAD specified for padstack PAD50X100 at (-1831.06 1801.46).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-1525.17 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-1564.54 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-1525.17 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-1564.54 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack SMD40_35 at (-1513.54 -413.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD40_35 at (-1573.54 -413.54).
    WARNING: Null REGULAR-PAD specified for padstack RECT55X65 at (-1618.54 -328.54).
    WARNING: Null REGULAR-PAD specified for padstack RECT55X65 at (-1508.54 -328.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD40_35 at (-1553.54 196.46).
    WARNING: Null REGULAR-PAD specified for padstack RECT55X65 at (-1613.54 286.46).
    WARNING: Null REGULAR-PAD specified for padstack RECT55X65 at (-1503.54 286.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD40_35 at (-1658.54 771.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD40_35 at (-1658.54 711.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ30 at (-1543.54 783.96).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ30 at (-1543.54 728.96).
    WARNING: Null REGULAR-PAD specified for padstack PAD50X125 at (-1536.02 886.46).
    WARNING: Null REGULAR-PAD specified for padstack PAD50X125 at (-1536.02 986.46).
    WARNING: Null REGULAR-PAD specified for padstack RE36X48 at (-1653.54 1025.96).
    WARNING: Null REGULAR-PAD specified for padstack RE36X48 at (-1653.54 896.96).
    WARNING: Null REGULAR-PAD specified for padstack PAD50X125 at (-1536.02 1086.46).
    WARNING: Null REGULAR-PAD specified for padstack PAD50X125 at (-1536.02 1186.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ30 at (-1716.04 1091.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ30 at (-1661.04 1091.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ30 at (-1716.04 1151.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ30 at (-1661.04 1151.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ30 at (-1716.04 1211.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ30 at (-1661.04 1211.46).
    WARNING: Null REGULAR-PAD specified for padstack PAD50X125 at (-1536.02 1286.46).
    WARNING: Null REGULAR-PAD specified for padstack PAD50X125 at (-1536.02 1386.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ30 at (-1716.04 1271.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ30 at (-1661.04 1271.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ30 at (-1716.04 1331.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ30 at (-1661.04 1331.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ30 at (-1716.04 1391.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ30 at (-1661.04 1391.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ30 at (-1716.04 1451.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ30 at (-1661.04 1451.46).
    WARNING: Null REGULAR-PAD specified for padstack PAD50X125 at (-1536.02 1486.46).
    WARNING: Null REGULAR-PAD specified for padstack PAD50X125 at (-1536.02 1586.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_31_35 at (-1588.54 1669.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ30 at (-1716.04 1511.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ30 at (-1661.04 1511.46).
    WARNING: Null REGULAR-PAD specified for padstack PAD50X100 at (-1681.06 1601.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1523.54 1766.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1523.54 1806.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_31_35 at (-1588.54 1828.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_31_35 at (-1588.54 1774.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_31_35 at (-1588.54 1723.46).
    WARNING: Null REGULAR-PAD specified for padstack PAD50X100 at (-1681.06 1701.46).
    WARNING: Null REGULAR-PAD specified for padstack PAD50X100 at (-1681.06 1801.46).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-1565.26 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-1525.89 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-1565.26 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-1525.89 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-1328.32 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-1367.69 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-1407.06 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-1446.43 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-1485.80 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-1328.32 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-1367.69 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-1407.06 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-1446.43 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-1485.80 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1388.54 -553.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1388.54 -513.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1348.54 -553.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1348.54 -513.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1498.23 -493.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1458.85 -493.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1318.23 -553.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1438.54 -278.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1438.54 -318.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1378.23 -83.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1338.85 -83.54).
    WARNING: Null REGULAR-PAD specified for padstack RECT25X20 at (-1368.54 -23.54).
    WARNING: Null REGULAR-PAD specified for padstack RECT25X20 at (-1328.54 -23.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1383.54 71.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1383.54 111.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1343.54 71.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1343.54 111.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1383.23 21.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1343.85 21.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1313.23 71.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD40_35 at (-1493.54 196.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1428.54 346.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1428.54 306.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1323.54 256.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1323.54 296.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1488.23 456.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1448.85 456.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1323.54 541.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1323.54 501.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1493.23 726.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1453.85 726.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD30_50 at (-1366.04 776.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD30_50 at (-1366.04 676.46).
    WARNING: Null REGULAR-PAD specified for padstack RE28X71 at (-1342.80 792.76).
    WARNING: Null REGULAR-PAD specified for padstack RECT60X110 at (-1417.60 738.43).
    WARNING: Null REGULAR-PAD specified for padstack PAD50X125 at (-1321.06 886.46).
    WARNING: Null REGULAR-PAD specified for padstack PAD50X125 at (-1321.06 986.46).
    WARNING: Null REGULAR-PAD specified for padstack RE28X71 at (-1342.80 840.01).
    WARNING: Null REGULAR-PAD specified for padstack RE40X71 at (-1342.80 891.19).
    WARNING: Null REGULAR-PAD specified for padstack RE40X71 at (-1342.80 956.15).
    WARNING: Null REGULAR-PAD specified for padstack PAD50X125 at (-1321.06 1086.46).
    WARNING: Null REGULAR-PAD specified for padstack PAD50X125 at (-1321.06 1186.46).
    WARNING: Null REGULAR-PAD specified for padstack RE40X71 at (-1342.80 1054.57).
    WARNING: Null REGULAR-PAD specified for padstack RE40X71 at (-1342.80 1153.00).
    WARNING: Null REGULAR-PAD specified for padstack RE40X71 at (-1342.80 1251.42).
    WARNING: Null REGULAR-PAD specified for padstack PAD50X125 at (-1321.06 1286.46).
    WARNING: Null REGULAR-PAD specified for padstack PAD50X125 at (-1321.06 1386.46).
    WARNING: Null REGULAR-PAD specified for padstack RE40X71 at (-1342.80 1349.85).
    WARNING: Null REGULAR-PAD specified for padstack RE40X71 at (-1342.80 1448.27).
    WARNING: Null REGULAR-PAD specified for padstack PAD50X125 at (-1321.06 1486.46).
    WARNING: Null REGULAR-PAD specified for padstack PAD50X125 at (-1321.06 1586.46).
    WARNING: Null REGULAR-PAD specified for padstack RE40X71 at (-1342.80 1645.13).
    WARNING: Null REGULAR-PAD specified for padstack RE40X71 at (-1342.80 1546.70).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_44_72 at (-1456.54 1741.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_44_32 at (-1456.54 1821.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_44_32 at (-1380.54 1821.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_44_32 at (-1380.54 1741.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1328.54 1836.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1328.54 1796.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1328.54 1726.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1328.54 1766.15).
    WARNING: Null REGULAR-PAD specified for padstack RECT60X110 at (-1417.60 1726.62).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-1486.52 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-1447.15 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-1407.78 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-1368.41 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-1329.04 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-1486.52 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-1447.15 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-1407.78 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-1368.41 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-1329.04 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-1170.84 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-1210.21 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-1249.58 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-1288.95 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-1170.84 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-1210.21 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-1249.58 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-1288.95 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1278.85 -553.54).
    WARNING: Null REGULAR-PAD specified for padstack RECT25X20 at (-1278.54 -603.54).
    WARNING: Null REGULAR-PAD specified for padstack RECT25X20 at (-1238.54 -603.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1218.54 -363.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1218.54 -323.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_32_36 at (-1180.54 -233.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_32_36 at (-1116.54 -233.54).
    WARNING: Null REGULAR-PAD specified for padstack RECT25X20 at (-1153.54 -233.54).
    WARNING: Null REGULAR-PAD specified for padstack RECT25X20 at (-1113.54 -233.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1248.85 -98.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1288.23 -98.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1248.85 -138.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1288.23 -138.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1178.85 -98.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1218.23 -98.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ_35 at (-1103.54 -163.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ_35 at (-1153.54 -163.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1108.54 71.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1108.54 111.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1183.23 176.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1143.85 176.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1273.85 71.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ30 at (-1158.54 63.96).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ30 at (-1158.54 118.96).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (-1105.94 117.05).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (-1105.94 65.87).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1178.54 396.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1183.54 241.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1183.54 281.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1198.85 321.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1238.23 321.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1198.85 361.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1238.23 361.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1198.85 281.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1238.23 281.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1138.23 231.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1098.85 231.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1138.23 271.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1098.85 271.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-1130.90 242.56).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-1130.90 262.25).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-1130.90 281.93).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-1130.90 301.62).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-1130.90 321.30).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-1130.90 340.99).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-1130.90 360.67).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-1130.90 380.36).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1178.54 436.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1283.54 541.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1283.54 501.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1208.85 541.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1248.23 541.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_25_TP at (-1208.54 436.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1153.54 681.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1153.54 721.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_32_36 at (-1203.54 654.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_32_36 at (-1203.54 718.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD40_35 at (-1213.54 666.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD40_35 at (-1273.54 666.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD40_50 at (-1296.04 776.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD30_50 at (-1291.04 676.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1203.23 906.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1163.85 906.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1203.23 946.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1163.85 946.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1203.23 1026.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1163.85 1026.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1203.23 986.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1163.85 986.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1203.23 986.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1163.85 986.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1203.23 906.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1163.85 906.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1203.23 946.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1163.85 946.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1203.23 1026.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1163.85 1026.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1203.23 1106.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1163.85 1106.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1203.23 1066.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1163.85 1066.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1203.23 1186.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1163.85 1186.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1203.23 1146.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1163.85 1146.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1203.23 1106.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1163.85 1106.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1203.23 1146.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1163.85 1146.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1203.23 1226.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1163.85 1226.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1203.23 1186.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1163.85 1186.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1203.23 1066.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1163.85 1066.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD120X100 at (-1113.54 1431.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD100X178 at (-1208.07 1456.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1203.23 1306.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1163.85 1306.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1163.85 1266.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1203.23 1266.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1283.54 1276.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1283.54 1316.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1243.54 1276.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1243.54 1316.15).
    WARNING: Null REGULAR-PAD specified for padstack PAD10X32 at (-1157.91 1657.40).
    WARNING: Null REGULAR-PAD specified for padstack PAD10X32 at (-1138.23 1657.40).
    WARNING: Null REGULAR-PAD specified for padstack PAD10X32 at (-1118.54 1657.40).
    WARNING: Null REGULAR-PAD specified for padstack SMD120X100 at (-1113.54 1691.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1128.85 1596.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1168.23 1596.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1098.23 1596.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_32_36 at (-1223.54 1619.46).
    WARNING: Null REGULAR-PAD specified for padstack PAD98X66_1 at (-1118.54 1716.46).
    WARNING: Null REGULAR-PAD specified for padstack PAD10X32 at (-1118.54 1775.52).
    WARNING: Null REGULAR-PAD specified for padstack PAD10X32 at (-1138.23 1775.52).
    WARNING: Null REGULAR-PAD specified for padstack PAD10X32 at (-1157.91 1775.52).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1198.85 1771.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1238.23 1771.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1198.85 1731.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1238.23 1731.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_32_36 at (-1223.54 1683.46).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-1289.67 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-1250.30 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-1210.93 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-1171.56 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-1132.19 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-1289.67 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-1250.30 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-1210.93 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-1171.56 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-1132.19 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-895.25 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-934.62 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-973.99 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-1013.36 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-1052.73 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-895.25 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-934.62 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-973.99 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-1013.36 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-1052.73 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack RECT80X90 at (-988.54 -598.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-893.54 -493.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-893.54 -453.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-933.54 -493.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-933.54 -453.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-973.54 -493.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-973.54 -453.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-973.54 -493.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-973.54 -453.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-933.54 -493.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-933.54 -453.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-893.54 -493.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-893.54 -453.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-973.54 -413.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-933.54 -413.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-893.54 -413.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_31_35 at (-1058.54 -485.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_31_35 at (-1058.54 -431.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ_35 at (-1058.54 -433.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ_35 at (-1058.54 -483.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-973.54 -373.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-933.54 -373.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-893.54 -373.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1023.85 -208.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1063.23 -208.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1023.85 -248.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1063.23 -248.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-919.01 -370.90).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-938.70 -370.90).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-958.38 -370.90).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-978.07 -370.90).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-997.75 -370.90).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-1017.44 -370.90).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-1050.90 -337.44).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-1050.90 -317.75).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-1050.90 -298.07).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-1050.90 -278.38).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-1050.90 -258.70).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-1050.90 -239.01).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-1050.90 -219.33).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ140NP at (-948.54 -268.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-948.54 -108.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-948.54 -68.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-988.54 -108.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-988.54 -68.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1028.54 -108.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1028.54 -68.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1068.54 -108.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1068.54 -68.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-948.54 -108.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-948.54 -68.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-988.54 -108.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-988.54 -68.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-1017.44 -166.18).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-997.75 -166.18).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-978.07 -166.18).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-958.38 -166.18).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-938.70 -166.18).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-919.01 -166.18).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-1050.90 -199.64).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-908.54 66.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-908.54 106.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1073.23 36.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1033.85 36.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1063.54 71.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1063.54 111.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ30 at (-958.54 58.96).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ30 at (-958.54 113.96).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-959.64 209.10).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-979.33 209.10).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-999.01 209.10).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-1018.70 209.10).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-1038.38 209.10).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-1058.07 209.10).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-1077.75 209.10).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-1097.44 209.10).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_25_TP at (-1013.54 116.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (-905.94 112.05).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (-905.94 60.87).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (-1031.14 65.87).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (-1031.14 91.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (-1031.14 117.05).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-928.85 401.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-968.23 401.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1058.54 421.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1058.54 381.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-928.85 241.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-968.23 241.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-928.85 361.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-968.23 361.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-928.85 281.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-968.23 281.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-928.85 321.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-968.23 321.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-926.18 380.36).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-926.18 360.67).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-926.18 340.99).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-926.18 321.30).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-926.18 301.62).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-926.18 281.93).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-926.18 262.25).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-926.18 242.56).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-1097.44 413.82).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-1077.75 413.82).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-1058.07 413.82).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-1038.38 413.82).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-1018.70 413.82).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-999.01 413.82).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-979.33 413.82).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-959.64 413.82).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ140NP at (-1028.54 311.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-983.23 586.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-943.85 586.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_31_35 at (-1058.54 584.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_31_35 at (-1058.54 638.46).
    WARNING: Null REGULAR-PAD specified for padstack S_RCT_1-55_X_0-60 at (-1059.84 586.46).
    WARNING: Null REGULAR-PAD specified for padstack S_RCT_1-55_X_0-60 at (-1059.84 536.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD120X100 at (-1048.54 781.46).
    WARNING: Null REGULAR-PAD specified for padstack S_RCT_1-55_X_0-60 at (-1059.84 686.46).
    WARNING: Null REGULAR-PAD specified for padstack S_RCT_1-55_X_0-60 at (-1059.84 636.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD120X100 at (-1048.54 1041.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD120X100 at (-853.54 911.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD100X178 at (-938.07 946.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD120X100 at (-853.54 1171.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-938.85 1216.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-978.23 1216.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-908.23 1081.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_32_36 at (-963.54 1168.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_32_36 at (-963.54 1104.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ_35 at (-1078.54 1256.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ_35 at (-1078.54 1206.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ_35 at (-1078.54 1256.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ_35 at (-1078.54 1206.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD100X178 at (-1049.01 1456.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD100X178 at (-908.07 1456.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-938.85 1256.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-978.23 1256.46).
    WARNING: Null REGULAR-PAD specified for padstack PAD10X32 at (-1098.85 1657.40).
    WARNING: Null REGULAR-PAD specified for padstack PAD10X32 at (-1079.17 1657.40).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-1058.85 1596.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_32_36 at (-923.54 1619.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_31_35 at (-1013.54 1599.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_31_35 at (-1013.54 1653.46).
    WARNING: Null REGULAR-PAD specified for padstack PAD10X32 at (-1079.17 1775.52).
    WARNING: Null REGULAR-PAD specified for padstack PAD10X32 at (-1098.85 1775.52).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-898.85 1771.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-938.23 1771.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-898.85 1731.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-938.23 1731.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_32_36 at (-923.54 1683.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_31_35 at (-1013.54 1699.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_31_35 at (-1013.54 1753.46).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-1092.82 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-1053.45 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-1014.08 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-974.71 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-935.34 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-895.97 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-1092.82 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-1053.45 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-1014.08 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-974.71 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-935.34 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-895.97 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-698.40 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-737.77 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-777.14 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-816.51 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-855.88 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-698.40 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-737.77 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-777.14 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-816.51 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-855.88 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack RECT80X90 at (-858.54 -598.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-853.54 -493.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-853.54 -453.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-853.54 -413.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_32_36 at (-773.54 -415.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-738.85 -303.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-778.23 -303.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-738.85 -263.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-778.23 -263.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-738.85 -223.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-778.23 -223.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-778.23 -303.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-738.85 -303.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-853.54 -373.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-873.23 -333.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-833.85 -333.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_32_36 at (-773.54 -351.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-846.18 -219.33).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-846.18 -239.01).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-846.18 -258.70).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-846.18 -278.38).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-846.18 -298.07).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-846.18 -317.75).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-846.18 -337.44).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-879.64 -370.90).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-899.33 -370.90).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-738.85 -143.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-778.23 -143.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-778.23 -183.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-738.85 -183.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_32_36 at (-743.54 -25.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_32_36 at (-743.54 -25.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-899.33 -166.18).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-879.64 -166.18).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-846.18 -199.64).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-753.23 206.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-713.85 206.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-863.54 66.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-863.54 106.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_32_36 at (-743.54 38.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_32_36 at (-743.54 38.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_25_TP at (-813.54 56.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (-831.14 60.87).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (-831.14 86.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (-831.14 112.05).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-863.23 291.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-823.85 291.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-863.23 331.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-823.85 331.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-753.23 246.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-713.85 246.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_32_36 at (-860.54 311.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_32_36 at (-796.54 311.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_32_36 at (-875.54 231.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_32_36 at (-811.54 231.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_31_35 at (-821.54 426.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_31_35 at (-875.54 426.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_32_36 at (-875.54 436.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_32_36 at (-811.54 436.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_32_36 at (-738.54 604.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_32_36 at (-738.54 604.46).
    WARNING: Null REGULAR-PAD specified for padstack S_RCT_1-55_X_0-60 at (-847.24 536.46).
    WARNING: Null REGULAR-PAD specified for padstack S_RCT_1-55_X_0-60 at (-847.24 586.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_32_36 at (-738.54 668.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_32_36 at (-738.54 668.46).
    WARNING: Null REGULAR-PAD specified for padstack S_RCT_1-55_X_0-60 at (-847.24 636.46).
    WARNING: Null REGULAR-PAD specified for padstack S_RCT_1-55_X_0-60 at (-847.24 686.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD100X178 at (-779.01 946.46).
    WARNING: Null REGULAR-PAD specified for padstack PAD98X66_1 at (-858.54 1201.46).
    WARNING: Null REGULAR-PAD specified for padstack PAD10X32 at (-897.91 1142.40).
    WARNING: Null REGULAR-PAD specified for padstack PAD10X32 at (-878.23 1142.40).
    WARNING: Null REGULAR-PAD specified for padstack PAD10X32 at (-858.54 1142.40).
    WARNING: Null REGULAR-PAD specified for padstack PAD10X32 at (-838.85 1142.40).
    WARNING: Null REGULAR-PAD specified for padstack PAD10X32 at (-819.17 1142.40).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-868.85 1081.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-833.23 1081.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-793.85 1081.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_31_35 at (-753.54 1089.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_31_35 at (-753.54 1143.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_31_35 at (-753.54 1194.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_31_35 at (-753.54 1248.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (-685.94 1235.87).
    WARNING: Null REGULAR-PAD specified for padstack PAD10X32 at (-819.17 1260.52).
    WARNING: Null REGULAR-PAD specified for padstack PAD10X32 at (-838.85 1260.52).
    WARNING: Null REGULAR-PAD specified for padstack PAD10X32 at (-858.54 1260.52).
    WARNING: Null REGULAR-PAD specified for padstack PAD10X32 at (-878.23 1260.52).
    WARNING: Null REGULAR-PAD specified for padstack PAD10X32 at (-897.91 1260.52).
    WARNING: Null REGULAR-PAD specified for padstack SMD120X100 at (-813.54 1426.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD100X178 at (-749.01 1456.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-688.23 1331.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (-685.94 1287.05).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (-685.94 1261.46).
    WARNING: Null REGULAR-PAD specified for padstack PAD10X32 at (-857.91 1657.40).
    WARNING: Null REGULAR-PAD specified for padstack PAD10X32 at (-838.23 1657.40).
    WARNING: Null REGULAR-PAD specified for padstack PAD10X32 at (-818.54 1657.40).
    WARNING: Null REGULAR-PAD specified for padstack PAD10X32 at (-798.85 1657.40).
    WARNING: Null REGULAR-PAD specified for padstack PAD10X32 at (-779.17 1657.40).
    WARNING: Null REGULAR-PAD specified for padstack SMD120X100 at (-813.54 1686.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-828.85 1596.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-868.23 1596.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-798.23 1596.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-758.85 1596.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_31_35 at (-713.54 1599.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_31_35 at (-713.54 1653.46).
    WARNING: Null REGULAR-PAD specified for padstack PAD98X66_1 at (-818.54 1716.46).
    WARNING: Null REGULAR-PAD specified for padstack PAD10X32 at (-779.17 1775.52).
    WARNING: Null REGULAR-PAD specified for padstack PAD10X32 at (-798.85 1775.52).
    WARNING: Null REGULAR-PAD specified for padstack PAD10X32 at (-818.54 1775.52).
    WARNING: Null REGULAR-PAD specified for padstack PAD10X32 at (-838.23 1775.52).
    WARNING: Null REGULAR-PAD specified for padstack PAD10X32 at (-857.91 1775.52).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-778.85 1776.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-818.23 1776.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-723.54 1816.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-723.54 1856.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-683.54 1816.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-683.54 1856.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_31_35 at (-713.54 1704.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_31_35 at (-713.54 1758.46).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-856.60 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-817.23 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-777.85 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-738.48 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-699.11 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-856.60 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-817.23 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-777.85 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-738.48 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-699.11 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-501.55 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-540.92 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-580.29 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-619.66 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-659.03 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-501.55 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-540.92 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-580.29 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-619.66 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-659.03 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_31_35 at (-489.26 -556.29).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_31_35 at (-489.26 -502.29).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ_35 at (-489.26 -504.29).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ_35 at (-489.26 -554.29).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-496.62 -408.19).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-508.23 -278.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-508.23 -318.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_32_36 at (-631.26 -304.29).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_32_36 at (-567.26 -304.29).
    WARNING: Null REGULAR-PAD specified for padstack RECT25X20 at (-609.26 -309.29).
    WARNING: Null REGULAR-PAD specified for padstack RECT25X20 at (-569.26 -309.29).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ_35 at (-544.26 -234.29).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ_35 at (-594.26 -234.29).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-496.62 -388.50).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-496.62 -368.82).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-496.62 -349.13).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-496.62 -329.45).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-496.62 -309.76).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-496.62 -290.08).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-496.62 -270.39).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-622.52 0.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-559.57 0.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-496.57 0.50).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-509.26 -173.98).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-509.26 -134.60).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-478.54 -13.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-633.23 -28.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-593.85 -28.54).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-622.52 32.00).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-591.07 32.00).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-559.57 32.00).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-528.07 32.00).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-496.57 32.00).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-622.52 63.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-622.52 189.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-591.07 63.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-591.07 189.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-559.57 63.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-559.57 189.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-528.07 63.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-528.07 189.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-496.57 63.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-496.57 189.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-654.01 189.45).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-654.01 63.47).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-654.01 31.97).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-633.23 21.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-593.85 21.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-478.54 26.15).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-622.52 221.00).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-591.07 221.00).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-591.07 252.44).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-559.57 221.00).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-528.07 221.00).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-528.07 252.44).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-496.57 221.00).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-654.01 252.44).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-654.01 220.95).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-622.52 390.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-559.57 390.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-496.57 390.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-622.52 422.00).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-591.07 422.00).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-559.57 422.00).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-528.07 422.00).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-496.57 422.00).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-622.52 453.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-622.52 579.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-622.52 611.00).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-591.07 453.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-591.07 579.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-591.07 611.00).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-559.57 453.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-559.57 579.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-559.57 611.00).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-528.07 453.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-528.07 579.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-528.07 611.00).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-496.57 453.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-496.57 579.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-496.57 611.00).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-654.01 610.95).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-654.01 579.45).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-654.01 453.47).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-654.01 421.97).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-628.85 616.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-668.23 616.46).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-591.07 642.44).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-528.07 642.44).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-654.01 642.44).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-658.23 831.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-618.85 831.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-488.85 776.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-528.23 776.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-678.54 741.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-678.54 781.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-573.54 801.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-573.54 761.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-628.85 656.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-668.23 656.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-548.23 641.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-508.85 641.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-618.54 801.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-618.54 761.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_25_TP at (-538.54 826.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (-483.54 793.86).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (-509.13 793.86).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (-509.13 719.06).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (-634.13 729.06).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (-608.54 729.06).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (-582.95 729.06).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (-582.95 803.86).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (-634.13 803.86).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-673.54 891.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-673.54 931.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-673.54 1006.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-673.54 1046.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-628.54 891.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-628.54 931.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-628.54 1006.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-628.54 1046.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ_35 at (-538.54 926.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ_35 at (-538.54 876.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_40_10 at (-541.19 861.27).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_40_10 at (-541.19 880.96).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_40_10 at (-541.19 900.65).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_40_10 at (-541.19 920.34).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_40_10 at (-541.19 940.03).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_40_10 at (-541.19 959.72).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_40_10 at (-541.19 979.41).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_40_10 at (-541.19 999.10).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_40_10 at (-541.19 1018.79).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_40_10 at (-541.19 1038.48).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (-669.13 999.06).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (-643.54 999.06).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (-617.95 999.06).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (-669.13 884.06).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (-643.54 884.06).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (-617.95 884.06).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (-617.95 958.86).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (-669.13 958.86).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-603.54 1241.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-483.23 1126.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-648.54 1241.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-543.54 1101.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-543.54 1141.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-663.23 1151.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-623.85 1151.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_40_10 at (-541.19 1058.17).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_40_10 at (-541.19 1077.86).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_40_10 at (-541.19 1097.55).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_40_10 at (-541.19 1117.24).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_40_10 at (-541.19 1136.93).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_40_10 at (-541.19 1156.62).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_40_10 at (-541.19 1176.31).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_40_10 at (-541.19 1196.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_40_10 at (-541.19 1215.69).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_40_10 at (-541.19 1235.38).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (-611.14 1235.87).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (-617.95 1073.86).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (-669.13 1073.86).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (-669.13 1114.06).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (-643.54 1114.06).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (-617.95 1114.06).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (-617.95 1188.86).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (-669.13 1188.86).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-603.54 1281.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-648.85 1331.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-598.54 1336.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-598.54 1376.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-648.54 1281.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-543.54 1311.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-543.54 1351.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_40_10 at (-541.19 1392.90).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_40_10 at (-541.19 1373.21).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_40_10 at (-541.19 1353.52).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_40_10 at (-541.19 1333.83).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_40_10 at (-541.19 1314.14).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_40_10 at (-541.19 1294.45).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_40_10 at (-541.19 1274.76).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_40_10 at (-541.19 1255.07).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (-611.14 1287.05).
    WARNING: Null REGULAR-PAD specified for padstack RECT80X90 at (-473.54 1531.46).
    WARNING: Null REGULAR-PAD specified for padstack RECT80X90 at (-603.54 1531.46).
    WARNING: Null REGULAR-PAD specified for padstack PAD_100X028 at (-508.64 1524.96).
    WARNING: Null REGULAR-PAD specified for padstack PAD_100X028 at (-558.64 1524.96).
    WARNING: Null REGULAR-PAD specified for padstack PAD_100X028 at (-608.64 1524.96).
    WARNING: Null REGULAR-PAD specified for padstack PAD_100X028 at (-658.64 1524.96).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-498.54 1816.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-498.54 1856.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-538.54 1856.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-538.54 1816.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-618.54 1856.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-618.54 1816.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-498.54 1856.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-498.54 1816.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-578.54 1856.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-578.54 1816.77).
    WARNING: Null REGULAR-PAD specified for padstack PAD_100X028 at (-508.64 1737.96).
    WARNING: Null REGULAR-PAD specified for padstack PAD_100X028 at (-558.64 1737.96).
    WARNING: Null REGULAR-PAD specified for padstack PAD_100X028 at (-608.64 1737.96).
    WARNING: Null REGULAR-PAD specified for padstack PAD_100X028 at (-658.64 1737.96).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-659.74 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-620.37 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-581.00 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-541.63 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-502.26 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-659.74 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-620.37 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-581.00 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-541.63 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-502.26 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-304.70 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-344.07 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-383.44 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-422.81 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-462.18 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-304.70 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-344.07 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-383.44 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-422.81 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-462.18 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-448.54 -628.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-448.54 -668.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-408.54 -628.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-408.54 -668.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-294.26 -563.98).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-294.26 -524.60).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-334.26 -563.98).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-334.26 -524.60).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-374.26 -563.98).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-374.26 -524.60).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-414.26 -563.98).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-414.26 -524.60).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-414.26 -563.98).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-414.26 -524.60).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-414.26 -483.98).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-414.26 -444.60).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-374.26 -563.98).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-374.26 -524.60).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-374.26 -483.98).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-374.26 -444.60).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-334.26 -563.98).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-334.26 -524.60).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-334.26 -483.98).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-334.26 -444.60).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-294.26 -483.98).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-294.26 -444.60).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-318.95 -409.29).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-279.57 -409.29).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-291.90 -408.19).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-325.36 -441.65).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-345.05 -441.65).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-364.73 -441.65).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-384.42 -441.65).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-404.10 -441.65).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-423.79 -441.65).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-443.47 -441.65).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-463.16 -441.65).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-468.85 -278.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-468.85 -318.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-463.16 -236.93).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-443.47 -236.93).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-423.79 -236.93).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-404.10 -236.93).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-384.42 -236.93).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-364.73 -236.93).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-345.05 -236.93).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-325.36 -236.93).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-291.90 -270.39).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-291.90 -290.08).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-291.90 -309.76).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-291.90 -329.45).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-291.90 -349.13).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-291.90 -368.82).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (-291.90 -388.50).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ140NP at (-394.26 -339.29).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-402.07 0.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-465.07 0.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-433.57 0.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-370.57 0.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-339.07 0.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-307.57 0.50).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-393.85 -38.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-433.23 -38.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-389.26 -173.98).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-389.26 -134.60).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-429.26 -173.98).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-429.26 -134.60).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-389.26 -173.98).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-389.26 -134.60).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-429.26 -173.98).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-429.26 -134.60).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-469.26 -173.98).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-469.26 -134.60).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-333.54 -3.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-293.23 -43.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-443.23 1.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-403.85 1.46).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-402.07 32.00).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-465.07 32.00).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-433.57 32.00).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-370.57 32.00).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-339.07 32.00).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-307.57 32.00).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-402.07 63.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-402.07 189.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-465.07 63.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-465.07 189.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-433.57 63.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-433.57 189.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-370.57 189.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-370.57 63.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-339.07 63.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-339.07 189.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-307.57 189.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-307.57 63.50).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-278.54 211.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-278.54 171.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-333.54 36.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-473.54 196.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-413.54 201.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-443.23 41.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-403.85 41.46).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-402.07 221.00).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-465.07 221.00).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-465.07 252.44).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-433.57 221.00).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-433.57 252.44).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-402.07 252.44).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-370.57 252.44).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-370.57 221.00).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-339.07 221.00).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-339.07 252.44).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-307.57 252.44).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-307.57 221.00).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-402.07 390.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-465.07 390.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-433.57 390.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-370.57 390.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-339.07 390.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-307.57 390.50).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-348.85 351.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-388.23 351.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-473.54 236.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-413.54 241.15).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-402.07 422.00).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-465.07 422.00).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-433.57 422.00).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-370.57 422.00).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-339.07 422.00).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-307.57 422.00).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-402.07 453.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-402.07 579.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-402.07 611.00).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-465.07 453.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-465.07 579.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-465.07 611.00).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-433.57 453.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-433.57 579.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-433.57 611.00).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-370.57 611.00).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-370.57 579.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-370.57 453.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-339.07 453.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-339.07 579.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-339.07 611.00).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-307.57 611.00).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-307.57 579.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-307.57 453.50).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-333.85 571.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-373.23 571.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-408.54 606.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-278.23 456.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-473.54 586.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-473.54 626.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-333.54 606.77).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-465.07 642.44).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-433.57 642.44).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-402.07 642.44).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-370.57 642.44).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-339.07 642.44).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-307.57 642.44).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-353.54 796.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-353.54 756.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-393.54 796.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-393.54 756.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-393.54 796.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-393.54 756.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-273.54 796.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-273.54 756.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-313.54 796.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-313.54 756.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-353.54 756.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-353.54 796.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-313.54 756.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-313.54 796.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-408.54 646.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-333.54 646.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (-457.95 793.86).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (-457.95 719.06).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-283.23 846.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-363.85 846.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-403.23 846.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-454.52 907.72).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-454.52 939.22).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-454.52 970.71).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-454.52 1002.21).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-454.52 1033.70).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-423.03 907.72).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-423.03 939.22).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-423.03 970.71).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-423.03 1002.21).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-423.03 1033.70).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-391.53 907.72).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-391.53 939.22).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-391.53 970.71).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-391.53 1002.21).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-391.53 1033.70).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-360.04 907.72).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-360.04 939.22).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-360.04 970.71).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-360.04 1002.21).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-360.04 1033.70).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-328.54 907.72).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-328.54 939.22).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-328.54 970.71).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-328.54 1002.21).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-328.54 1033.70).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-297.04 907.72).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-297.04 939.22).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-297.04 970.71).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-297.04 1002.21).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-297.04 1033.70).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-443.85 1126.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-333.85 1126.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-373.23 1126.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-283.23 1126.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-454.52 1187.72).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-454.52 1219.22).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-423.03 1187.72).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-423.03 1219.22).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-391.53 1187.72).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-391.53 1219.22).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-360.04 1187.72).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-360.04 1219.22).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-328.54 1187.72).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-328.54 1219.22).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-297.04 1187.72).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-297.04 1219.22).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-454.52 1065.20).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-423.03 1065.20).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-391.53 1065.20).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-360.04 1065.20).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-328.54 1065.20).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-297.04 1065.20).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-308.23 1436.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-373.85 1436.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-413.23 1436.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-454.52 1250.71).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-454.52 1282.21).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-454.52 1313.70).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-454.52 1345.20).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-423.03 1250.71).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-423.03 1282.21).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-423.03 1313.70).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-423.03 1345.20).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-391.53 1250.71).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-391.53 1282.21).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-391.53 1313.70).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-391.53 1345.20).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-360.04 1250.71).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-360.04 1282.21).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-360.04 1313.70).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-360.04 1345.20).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-328.54 1250.71).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-328.54 1282.21).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-328.54 1313.70).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-328.54 1345.20).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-297.04 1250.71).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-297.04 1282.21).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-297.04 1313.70).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-297.04 1345.20).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-358.54 1611.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-358.54 1651.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-398.54 1611.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-398.54 1651.15).
    WARNING: Null REGULAR-PAD specified for padstack PAD_100X028 at (-308.64 1524.96).
    WARNING: Null REGULAR-PAD specified for padstack PAD_100X028 at (-358.64 1524.96).
    WARNING: Null REGULAR-PAD specified for padstack PAD_100X028 at (-408.64 1524.96).
    WARNING: Null REGULAR-PAD specified for padstack PAD_100X028 at (-458.64 1524.96).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-293.54 1816.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-293.54 1856.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-458.54 1856.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-458.54 1816.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-293.54 1856.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-293.54 1816.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-333.54 1816.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-333.54 1856.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-373.54 1816.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-373.54 1856.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-413.54 1816.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-413.54 1856.15).
    WARNING: Null REGULAR-PAD specified for padstack PAD_100X028 at (-308.64 1737.96).
    WARNING: Null REGULAR-PAD specified for padstack PAD_100X028 at (-358.64 1737.96).
    WARNING: Null REGULAR-PAD specified for padstack PAD_100X028 at (-408.64 1737.96).
    WARNING: Null REGULAR-PAD specified for padstack PAD_100X028 at (-458.64 1737.96).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-462.89 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-423.52 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-384.15 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-344.78 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-305.41 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-462.89 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-423.52 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-384.15 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-344.78 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-305.41 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-107.85 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-147.22 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-186.59 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-225.96 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-265.33 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-107.85 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-147.22 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-186.59 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-225.96 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-265.33 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-263.54 -628.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-263.54 -668.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-173.54 -628.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-173.54 -668.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-133.54 -628.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-133.54 -668.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-68.54 -628.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-68.54 -668.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-133.54 -668.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-133.54 -628.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-173.54 -668.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-173.54 -628.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-68.54 -668.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-68.54 -628.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-73.23 -548.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-73.23 -448.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-73.23 -498.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_32_36 at (-224.26 -486.29).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_32_36 at (-224.26 -422.29).
    WARNING: Null REGULAR-PAD specified for padstack S_RCT_1-55_X_0-60 at (-54.84 -548.54).
    WARNING: Null REGULAR-PAD specified for padstack S_RCT_1-55_X_0-60 at (-54.84 -498.54).
    WARNING: Null REGULAR-PAD specified for padstack S_RCT_1-55_X_0-60 at (-54.84 -448.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-184.57 -294.29).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-223.95 -294.29).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-184.57 -374.29).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-223.95 -374.29).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-184.57 -334.29).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-223.95 -334.29).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-184.57 -294.29).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-223.95 -294.29).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-184.57 -214.29).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-223.95 -214.29).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-223.95 -374.29).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-184.57 -374.29).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-223.95 -254.29).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-184.57 -254.29).
    WARNING: Null REGULAR-PAD specified for padstack S_RCT_1-55_X_0-60 at (-54.84 -398.54).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-276.07 0.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-244.57 0.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-213.11 0.50).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-178.54 -3.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-253.85 -43.54).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-276.07 32.00).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-244.57 32.00).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-276.07 63.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-276.07 189.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-244.57 189.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-244.57 63.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-213.11 32.00).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-213.11 63.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-213.11 189.50).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-238.54 211.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-238.54 171.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-178.54 36.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-208.85 61.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-248.23 61.46).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-276.07 221.00).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-276.07 252.44).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-244.57 252.44).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-244.57 221.00).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-213.11 221.00).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-213.11 252.44).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-276.07 390.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-244.57 390.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-213.11 390.50).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-153.23 311.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-113.85 311.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-113.85 271.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-153.23 271.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-113.85 311.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-153.23 311.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-153.23 231.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-113.85 231.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-153.23 271.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-113.85 271.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-93.23 361.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-93.23 401.46).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-276.07 422.00).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-244.57 422.00).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-276.07 453.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-276.07 579.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-276.07 611.00).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-244.57 611.00).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-244.57 579.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-244.57 453.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-213.11 422.00).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-213.11 453.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-213.11 579.50).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-213.11 611.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-193.23 616.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-153.85 616.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-213.85 571.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-253.23 571.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-238.85 456.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ_35 at (-133.54 556.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ_35 at (-133.54 506.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ_35 at (-133.54 556.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ_35 at (-133.54 506.46).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-276.07 642.44).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-244.57 642.44).
    WARNING: Null REGULAR-PAD specified for padstack PAD16CIR at (-213.11 642.44).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-98.85 826.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-138.23 826.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-98.85 746.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-138.23 746.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-98.85 666.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-138.23 666.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-98.85 786.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-138.23 786.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-98.85 706.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-138.23 706.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-98.85 786.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-138.23 786.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-98.85 706.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-138.23 706.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-98.85 746.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-138.23 746.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-98.85 666.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-138.23 666.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-233.54 796.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-233.54 756.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-193.54 756.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-193.54 796.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-243.85 846.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-143.54 1031.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-143.54 991.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-143.54 911.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-143.54 951.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-265.55 907.72).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-265.55 939.22).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-265.55 970.71).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-265.55 1002.21).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-265.55 1033.70).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-234.05 907.72).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-234.05 939.22).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-234.05 970.71).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-234.05 1002.21).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-234.05 1033.70).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-202.56 907.72).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-202.56 939.22).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-202.56 970.71).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-202.56 1002.21).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-202.56 1033.70).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-84.52 907.72).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-84.52 939.22).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-84.52 970.71).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-84.52 1002.21).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-84.52 1033.70).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-143.54 1191.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-143.54 1231.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-243.85 1126.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-265.55 1187.72).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-265.55 1219.22).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-234.05 1187.72).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-234.05 1219.22).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-202.56 1187.72).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-202.56 1219.22).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-265.55 1065.20).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-234.05 1065.20).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-202.56 1065.20).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-84.52 1187.72).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-84.52 1219.22).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-84.52 1065.20).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-143.54 1316.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-143.54 1276.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-268.85 1436.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-265.55 1250.71).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-265.55 1282.21).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-265.55 1313.70).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-265.55 1345.20).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-234.05 1250.71).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-234.05 1282.21).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-234.05 1313.70).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-234.05 1345.20).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-202.56 1250.71).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-202.56 1282.21).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-202.56 1313.70).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-202.56 1345.20).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-84.52 1250.71).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-84.52 1282.21).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-84.52 1313.70).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-84.52 1345.20).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-208.54 1611.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-208.54 1651.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-143.85 1561.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-183.23 1561.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-163.54 1646.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-163.54 1606.77).
    WARNING: Null REGULAR-PAD specified for padstack R027X010S at (-92.91 1651.30).
    WARNING: Null REGULAR-PAD specified for padstack R027X010S at (-108.38 1616.15).
    WARNING: Null REGULAR-PAD specified for padstack R027X010S at (-108.38 1596.46).
    WARNING: Null REGULAR-PAD specified for padstack R027X010S at (-108.38 1576.77).
    WARNING: Null REGULAR-PAD specified for padstack R027X010S at (-92.91 1541.62).
    WARNING: Null REGULAR-PAD specified for padstack PAD_100X028 at (-108.64 1524.96).
    WARNING: Null REGULAR-PAD specified for padstack PAD_100X028 at (-158.64 1524.96).
    WARNING: Null REGULAR-PAD specified for padstack PAD_100X028 at (-208.64 1524.96).
    WARNING: Null REGULAR-PAD specified for padstack PAD_100X028 at (-258.64 1524.96).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-168.54 1856.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-168.54 1816.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-88.54 1856.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-88.54 1816.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-128.54 1856.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-128.54 1816.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-253.54 1816.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-253.54 1856.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-213.54 1816.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-213.54 1856.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_32_36 at (-90.54 1726.46).
    WARNING: Null REGULAR-PAD specified for padstack PAD_100X028 at (-108.64 1737.96).
    WARNING: Null REGULAR-PAD specified for padstack PAD_100X028 at (-158.64 1737.96).
    WARNING: Null REGULAR-PAD specified for padstack PAD_100X028 at (-208.64 1737.96).
    WARNING: Null REGULAR-PAD specified for padstack PAD_100X028 at (-258.64 1737.96).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-266.04 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-226.67 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-187.30 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-147.93 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-108.56 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-266.04 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-226.67 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-187.30 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-147.93 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-108.56 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (128.37 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (89.00 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (49.63 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (10.26 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-29.11 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-68.48 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (128.37 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (89.00 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (49.63 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (10.26 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-29.11 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-68.48 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (11.46 -628.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (11.46 -668.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-28.54 -628.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-28.54 -668.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (51.46 -628.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (51.46 -668.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (131.46 -628.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (131.46 -668.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (91.46 -628.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (91.46 -668.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-28.54 -668.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-28.54 -628.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (51.46 -668.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (51.46 -628.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (11.46 -668.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (11.46 -628.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-33.85 -548.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (136.77 -548.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-33.85 -448.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-33.85 -498.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-3.23 -498.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (36.15 -498.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (141.46 -493.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (141.46 -453.85).
    WARNING: Null REGULAR-PAD specified for padstack RECT25X20 at (91.46 -448.54).
    WARNING: Null REGULAR-PAD specified for padstack RECT25X20 at (91.46 -408.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (131.77 -198.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (131.77 -198.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (91.46 -253.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (91.46 -293.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-13.85 -343.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-53.23 -343.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-53.23 -263.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-13.85 -263.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-53.23 -263.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-13.85 -263.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-53.23 -303.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-13.85 -303.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (91.46 -323.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (91.46 -363.23).
    WARNING: Null REGULAR-PAD specified for padstack RECT35X45 at (39.37 -273.26).
    WARNING: Null REGULAR-PAD specified for padstack RECT35X45 at (39.37 -333.82).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (11.46 -138.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (11.46 -98.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (51.46 -138.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (51.46 -98.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (131.46 -138.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (131.46 -98.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (51.46 -138.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (51.46 -98.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (91.46 -138.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (91.46 -98.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (91.46 -138.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (91.46 -98.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (131.46 -138.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (131.46 -98.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (125.99 0.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (94.49 0.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (63.00 0.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (31.50 0.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (0.00 0.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (131.77 186.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (116.77 131.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (125.99 31.50).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (94.49 31.50).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (63.00 31.50).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (31.50 31.50).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (0.00 31.50).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (125.99 63.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (94.49 63.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (63.00 63.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (31.50 63.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (0.00 63.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (125.99 94.49).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (94.49 94.49).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (63.00 94.49).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (31.50 94.49).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (0.00 94.49).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (125.99 125.99).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (94.49 125.99).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (63.00 125.99).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (31.50 125.99).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (0.00 125.99).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (125.99 157.48).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (94.49 157.48).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (63.00 157.48).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (31.50 157.48).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (0.00 157.48).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (125.99 188.98).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (94.49 188.98).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (63.00 188.98).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (31.50 188.98).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (0.00 188.98).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (125.99 220.48).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (94.49 220.48).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (63.00 220.48).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (31.50 220.48).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (0.00 220.48).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-53.85 361.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-53.85 401.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (131.77 251.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (131.77 411.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (131.77 371.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (125.99 251.97).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (94.49 251.97).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (63.00 251.97).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (31.50 251.97).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (0.00 251.97).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (125.99 283.47).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (94.49 283.47).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (63.00 283.47).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (31.50 283.47).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (0.00 283.47).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (125.99 314.96).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (94.49 314.96).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (63.00 314.96).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (31.50 314.96).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (0.00 314.96).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (125.99 346.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (94.49 346.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (63.00 346.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (31.50 346.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (0.00 346.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (125.99 377.96).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (94.49 377.96).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (63.00 377.96).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (31.50 377.96).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (0.00 377.96).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (125.99 409.45).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (94.49 409.45).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (63.00 409.45).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (31.50 409.45).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (0.00 409.45).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (131.77 471.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (131.77 511.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (125.99 440.95).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (94.49 440.95).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (63.00 440.95).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (31.50 440.95).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (0.00 440.95).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (125.99 472.44).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (94.49 472.44).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (63.00 472.44).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (31.50 472.44).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (0.00 472.44).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (125.99 503.94).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (94.49 503.94).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (63.00 503.94).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (31.50 503.94).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (0.00 503.94).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (125.99 535.44).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (94.49 535.44).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (63.00 535.44).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (31.50 535.44).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (0.00 535.44).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (125.99 566.93).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (94.49 566.93).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (63.00 566.93).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (31.50 566.93).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (0.00 566.93).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (125.99 598.43).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (94.49 598.43).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (63.00 598.43).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (31.50 598.43).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (0.00 598.43).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (125.99 629.92).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (94.49 629.92).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (63.00 629.92).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (31.50 629.92).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (0.00 629.92).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (125.99 661.42).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (94.49 661.42).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (63.00 661.42).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (31.50 661.42).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (0.00 661.42).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (125.99 692.92).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (94.49 692.92).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (63.00 692.92).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (31.50 692.92).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (0.00 692.92).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1.15 846.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-38.23 846.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (46.77 846.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (86.15 846.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-53.03 907.72).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-53.03 939.22).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-53.03 970.71).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-53.03 1002.21).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-53.03 1033.70).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-21.53 907.72).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-21.53 939.22).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-21.53 970.71).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-21.53 1002.21).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-21.53 1033.70).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (9.96 907.72).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (9.96 939.22).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (9.96 970.71).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (9.96 1002.21).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (9.96 1033.70).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (41.46 907.72).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (41.46 939.22).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (41.46 970.71).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (41.46 1002.21).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (41.46 1033.70).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (72.96 907.72).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (72.96 939.22).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (72.96 970.71).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (72.96 1002.21).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (72.96 1033.70).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (104.45 907.72).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (104.45 939.22).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (104.45 970.71).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (104.45 1002.21).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (104.45 1033.70).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (11.15 1126.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-28.23 1126.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (91.77 1126.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (131.15 1126.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-53.03 1187.72).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-53.03 1219.22).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-21.53 1187.72).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-21.53 1219.22).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (9.96 1187.72).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (9.96 1219.22).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (41.46 1187.72).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (41.46 1219.22).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (72.96 1187.72).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (72.96 1219.22).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (104.45 1187.72).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (104.45 1219.22).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-53.03 1065.20).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-21.53 1065.20).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (9.96 1065.20).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (41.46 1065.20).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (72.96 1065.20).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (104.45 1065.20).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (101.77 1431.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (141.15 1431.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (16.15 1431.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-23.23 1431.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-53.03 1250.71).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-53.03 1282.21).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-53.03 1313.70).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-53.03 1345.20).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-21.53 1250.71).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-21.53 1282.21).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-21.53 1313.70).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (-21.53 1345.20).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (9.96 1250.71).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (9.96 1282.21).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (9.96 1313.70).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (9.96 1345.20).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (41.46 1250.71).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (41.46 1282.21).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (41.46 1313.70).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (41.46 1345.20).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (72.96 1250.71).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (72.96 1282.21).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (72.96 1313.70).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (72.96 1345.20).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (104.45 1250.71).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (104.45 1282.21).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (104.45 1313.70).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (104.45 1345.20).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (76.15 1586.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (36.77 1586.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_25_TP at (36.46 1631.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_25_TP at (1.46 1506.46).
    WARNING: Null REGULAR-PAD specified for padstack R027X010S at (-73.23 1651.30).
    WARNING: Null REGULAR-PAD specified for padstack R027X010S at (-73.23 1541.62).
    WARNING: Null REGULAR-PAD specified for padstack R027X010S at (-53.54 1541.62).
    WARNING: Null REGULAR-PAD specified for padstack R027X010S at (-33.85 1541.62).
    WARNING: Null REGULAR-PAD specified for padstack R027X010S at (-14.17 1541.62).
    WARNING: Null REGULAR-PAD specified for padstack R027X010S at (1.30 1576.77).
    WARNING: Null REGULAR-PAD specified for padstack R027X010S at (1.30 1596.46).
    WARNING: Null REGULAR-PAD specified for padstack R027X010S at (1.30 1616.15).
    WARNING: Null REGULAR-PAD specified for padstack R027X010S at (-14.17 1651.30).
    WARNING: Null REGULAR-PAD specified for padstack R027X010S at (-33.85 1651.30).
    WARNING: Null REGULAR-PAD specified for padstack R027X010S at (-53.54 1651.30).
    WARNING: Null REGULAR-PAD specified for padstack PAD_100X028 at (91.36 1524.96).
    WARNING: Null REGULAR-PAD specified for padstack PAD_100X028 at (41.36 1524.96).
    WARNING: Null REGULAR-PAD specified for padstack PAD_100X028 at (-8.64 1524.96).
    WARNING: Null REGULAR-PAD specified for padstack PAD_100X028 at (-58.64 1524.96).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (71.46 1856.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (71.46 1816.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (31.46 1816.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (31.46 1856.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-48.54 1816.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-48.54 1856.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-8.54 1816.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (-8.54 1856.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (111.46 1856.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (111.46 1816.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_32_36 at (-26.54 1726.46).
    WARNING: Null REGULAR-PAD specified for padstack PAD_100X028 at (91.36 1737.96).
    WARNING: Null REGULAR-PAD specified for padstack PAD_100X028 at (41.36 1737.96).
    WARNING: Null REGULAR-PAD specified for padstack PAD_100X028 at (-8.64 1737.96).
    WARNING: Null REGULAR-PAD specified for padstack PAD_100X028 at (-58.64 1737.96).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-69.19 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (-29.82 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (9.55 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (48.92 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (88.29 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (127.66 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-69.19 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (-29.82 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (9.55 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (48.92 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (88.29 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (127.66 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (325.22 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (285.85 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (246.48 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (207.11 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (167.74 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (325.22 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (285.85 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (246.48 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (207.11 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (167.74 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (171.46 -628.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (171.46 -668.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (296.15 -398.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (256.77 -398.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (296.15 -448.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (256.77 -448.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (296.15 -498.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (256.77 -498.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (296.15 -548.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (256.77 -548.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (176.15 -548.54).
    WARNING: Null REGULAR-PAD specified for padstack S_RCT_1-55_X_0-60 at (275.16 -548.54).
    WARNING: Null REGULAR-PAD specified for padstack S_RCT_1-55_X_0-60 at (275.16 -498.54).
    WARNING: Null REGULAR-PAD specified for padstack S_RCT_1-55_X_0-60 at (275.16 -448.54).
    WARNING: Null REGULAR-PAD specified for padstack S_RCT_1-55_X_0-60 at (157.76 -448.54).
    WARNING: Null REGULAR-PAD specified for padstack S_RCT_1-55_X_0-60 at (157.76 -498.54).
    WARNING: Null REGULAR-PAD specified for padstack S_RCT_1-55_X_0-60 at (157.76 -548.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (341.46 -253.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (341.46 -293.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (171.15 -198.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (171.15 -198.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (341.46 -323.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (341.46 -363.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD40_35 at (146.46 -273.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD40_35 at (146.46 -333.54).
    WARNING: Null REGULAR-PAD specified for padstack RECT35X45 at (289.37 -273.26).
    WARNING: Null REGULAR-PAD specified for padstack RECT35X45 at (289.37 -333.82).
    WARNING: Null REGULAR-PAD specified for padstack RECT35X45 at (143.55 -273.26).
    WARNING: Null REGULAR-PAD specified for padstack RECT35X45 at (143.55 -333.82).
    WARNING: Null REGULAR-PAD specified for padstack S_RCT_1-55_X_0-60 at (275.16 -398.54).
    WARNING: Null REGULAR-PAD specified for padstack S_RCT_1-55_X_0-60 at (157.76 -398.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_25_TP at (201.46 -228.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (291.46 -138.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (291.46 -98.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (291.46 -138.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (291.46 -98.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (251.46 -138.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (251.46 -98.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (211.46 -138.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (211.46 -98.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (331.46 -138.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (331.46 -98.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (331.46 -138.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (331.46 -98.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (211.46 -98.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (211.46 -138.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (171.46 -98.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (171.46 -138.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (171.46 -98.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (171.46 -138.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (251.46 -138.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (251.46 -98.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (314.96 0.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (283.47 0.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (251.97 0.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (220.48 0.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (188.98 0.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (157.48 0.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (171.15 186.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (281.46 216.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (211.46 181.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (211.46 221.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (341.46 211.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (316.46 171.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (316.46 131.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (251.46 171.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (251.46 131.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (156.15 131.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (314.96 31.50).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (283.47 31.50).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (251.97 31.50).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (220.48 31.50).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (188.98 31.50).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (157.48 31.50).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (314.96 63.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (283.47 63.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (251.97 63.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (220.48 63.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (188.98 63.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (157.48 63.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (314.96 94.49).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (283.47 94.49).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (251.97 94.49).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (220.48 94.49).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (188.98 94.49).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (157.48 94.49).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (314.96 125.99).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (283.47 125.99).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (251.97 125.99).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (220.48 125.99).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (188.98 125.99).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (157.48 125.99).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (314.96 157.48).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (283.47 157.48).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (251.97 157.48).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (220.48 157.48).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (188.98 157.48).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (157.48 157.48).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (157.48 188.98).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (314.96 220.48).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (283.47 220.48).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (251.97 220.48).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (220.48 220.48).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (157.48 220.48).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (181.46 296.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (181.46 336.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (281.46 256.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (341.46 251.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (251.15 366.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (211.77 366.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (251.15 251.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (211.77 251.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (171.15 251.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (171.15 411.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (171.15 371.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (314.96 251.97).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (283.47 251.97).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (251.97 251.97).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (220.48 251.97).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (157.48 251.97).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (314.96 283.47).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (283.47 283.47).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (251.97 283.47).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (220.48 283.47).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (157.48 283.47).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (314.96 314.96).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (283.47 314.96).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (251.97 314.96).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (220.48 314.96).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (157.48 314.96).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (314.96 346.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (283.47 346.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (251.97 346.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (220.48 346.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (157.48 346.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (314.96 377.96).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (283.47 377.96).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (251.97 377.96).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (220.48 377.96).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (157.48 377.96).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (314.96 409.45).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (283.47 409.45).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (251.97 409.45).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (220.48 409.45).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (157.48 409.45).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (281.46 441.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (281.46 481.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (281.46 511.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (281.46 551.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (251.15 441.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (211.77 441.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (341.46 441.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (341.46 481.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (221.46 516.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (221.46 476.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (321.46 521.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (321.46 561.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (171.15 471.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (171.15 511.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (314.96 440.95).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (283.47 440.95).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (251.97 440.95).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (220.48 440.95).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (157.48 440.95).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (314.96 472.44).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (283.47 472.44).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (251.97 472.44).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (220.48 472.44).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (157.48 472.44).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (157.48 503.94).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (314.96 535.44).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (283.47 535.44).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (251.97 535.44).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (220.48 535.44).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (188.98 535.44).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (157.48 535.44).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (314.96 566.93).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (283.47 566.93).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (251.97 566.93).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (220.48 566.93).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (188.98 566.93).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (157.48 566.93).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (314.96 598.43).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (283.47 598.43).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (251.97 598.43).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (220.48 598.43).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (188.98 598.43).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (157.48 598.43).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (314.96 629.92).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (283.47 629.92).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (251.97 629.92).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (220.48 629.92).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (188.98 629.92).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (157.48 629.92).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (336.46 831.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (336.46 791.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (251.46 826.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (251.46 786.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (211.46 826.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (211.46 786.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (211.46 826.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (211.46 786.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (171.46 826.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (171.46 786.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (171.46 826.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (171.46 786.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (291.46 826.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (291.46 786.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (251.46 826.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (251.46 786.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (314.96 661.42).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (283.47 661.42).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (251.97 661.42).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (220.48 661.42).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (188.98 661.42).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (157.48 661.42).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (314.96 692.92).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (283.47 692.92).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (251.97 692.92).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (220.48 692.92).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (188.98 692.92).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (157.48 692.92).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (321.77 956.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (321.77 906.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_40_10 at (254.11 861.27).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_40_10 at (254.11 880.96).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_40_10 at (254.11 900.65).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_40_10 at (254.11 920.34).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_40_10 at (254.11 1038.48).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_40_10 at (254.11 1018.79).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_40_10 at (254.11 999.10).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_40_10 at (254.11 979.41).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_40_10 at (254.11 959.72).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_40_10 at (254.11 940.03).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (135.95 907.72).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (135.95 939.22).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (135.95 970.71).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (135.95 1002.21).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (135.95 1033.70).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (167.44 907.72).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (167.44 939.22).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (167.44 970.71).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (167.44 1002.21).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (167.44 1033.70).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_28_12 at (315.12 905.87).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_28_12 at (315.12 931.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_28_12 at (315.12 957.05).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (286.15 1106.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (246.77 1106.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (286.15 1066.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (246.77 1066.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (291.77 1241.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (331.15 1241.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_40_10 at (254.11 1235.38).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_40_10 at (254.11 1215.69).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_40_10 at (254.11 1196.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_40_10 at (254.11 1176.31).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_40_10 at (254.11 1156.62).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_40_10 at (254.11 1136.93).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_40_10 at (254.11 1117.24).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_40_10 at (254.11 1097.55).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_40_10 at (254.11 1077.86).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_40_10 at (254.11 1058.17).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (135.95 1187.72).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (135.95 1219.22).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (167.44 1187.72).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (167.44 1219.22).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (135.95 1065.20).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (167.44 1065.20).
    WARNING: Null REGULAR-PAD specified for padstack R054X011S at (359.10 1447.88).
    WARNING: Null REGULAR-PAD specified for padstack R054X011S at (359.10 1428.19).
    WARNING: Null REGULAR-PAD specified for padstack R054X011S at (359.10 1408.51).
    WARNING: Null REGULAR-PAD specified for padstack R054X011S at (359.10 1388.82).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (291.77 1281.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (331.15 1281.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (346.77 1411.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (346.77 1451.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_40_10 at (254.11 1392.90).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_40_10 at (254.11 1373.21).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_40_10 at (254.11 1353.52).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_40_10 at (254.11 1333.83).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_40_10 at (254.11 1314.14).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_40_10 at (254.11 1294.45).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_40_10 at (254.11 1274.76).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_40_10 at (254.11 1255.07).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (135.95 1250.71).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (135.95 1282.21).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (135.95 1313.70).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (135.95 1345.20).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (167.44 1250.71).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (167.44 1282.21).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (167.44 1313.70).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_18 at (167.44 1345.20).
    WARNING: Null REGULAR-PAD specified for padstack R054X011S at (359.10 1644.73).
    WARNING: Null REGULAR-PAD specified for padstack R054X011S at (359.10 1625.04).
    WARNING: Null REGULAR-PAD specified for padstack R054X011S at (359.10 1605.36).
    WARNING: Null REGULAR-PAD specified for padstack R054X011S at (359.10 1585.67).
    WARNING: Null REGULAR-PAD specified for padstack R054X011S at (359.10 1565.99).
    WARNING: Null REGULAR-PAD specified for padstack R054X011S at (359.10 1546.30).
    WARNING: Null REGULAR-PAD specified for padstack R054X011S at (359.10 1526.62).
    WARNING: Null REGULAR-PAD specified for padstack R054X011S at (359.10 1506.93).
    WARNING: Null REGULAR-PAD specified for padstack R054X011S at (359.10 1487.25).
    WARNING: Null REGULAR-PAD specified for padstack R054X011S at (359.10 1467.56).
    WARNING: Null REGULAR-PAD specified for padstack PAD_100X028 at (291.36 1524.96).
    WARNING: Null REGULAR-PAD specified for padstack PAD_100X028 at (241.36 1524.96).
    WARNING: Null REGULAR-PAD specified for padstack PAD_100X028 at (191.36 1524.96).
    WARNING: Null REGULAR-PAD specified for padstack PAD_100X028 at (141.36 1524.96).
    WARNING: Null REGULAR-PAD specified for padstack R054X011S at (359.10 1684.10).
    WARNING: Null REGULAR-PAD specified for padstack R054X011S at (359.10 1664.41).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (151.46 1856.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (151.46 1816.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (191.46 1816.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (191.46 1856.15).
    WARNING: Null REGULAR-PAD specified for padstack PAD_100X028 at (291.36 1737.96).
    WARNING: Null REGULAR-PAD specified for padstack PAD_100X028 at (241.36 1737.96).
    WARNING: Null REGULAR-PAD specified for padstack PAD_100X028 at (191.36 1737.96).
    WARNING: Null REGULAR-PAD specified for padstack PAD_100X028 at (141.36 1737.96).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (167.03 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (206.40 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (245.77 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (285.14 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (324.51 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (167.03 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (206.40 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (245.77 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (285.14 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (324.51 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (522.07 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (482.70 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (443.33 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (403.96 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (364.59 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (522.07 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (482.70 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (443.33 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (403.96 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (364.59 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (451.46 -628.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (451.46 -668.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (491.46 -628.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (491.46 -668.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (546.46 -668.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (546.46 -628.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (506.15 -548.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (466.77 -548.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (466.46 -493.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (466.46 -453.85).
    WARNING: Null REGULAR-PAD specified for padstack RECT25X20 at (421.46 -453.54).
    WARNING: Null REGULAR-PAD specified for padstack RECT25X20 at (421.46 -413.54).
    WARNING: Null REGULAR-PAD specified for padstack S_RCT_1-55_X_0-60 at (487.76 -448.54).
    WARNING: Null REGULAR-PAD specified for padstack S_RCT_1-55_X_0-60 at (487.76 -498.54).
    WARNING: Null REGULAR-PAD specified for padstack S_RCT_1-55_X_0-60 at (487.76 -548.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (531.46 -188.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (531.46 -228.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD40_35 at (396.46 -273.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD40_35 at (396.46 -333.54).
    WARNING: Null REGULAR-PAD specified for padstack RECT35X45 at (393.55 -273.26).
    WARNING: Null REGULAR-PAD specified for padstack RECT35X45 at (393.55 -333.82).
    WARNING: Null REGULAR-PAD specified for padstack S_RCT_1-55_X_0-60 at (487.76 -398.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (521.46 -98.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (521.46 -138.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (491.46 -98.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (491.46 -138.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (481.46 -98.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (481.46 -138.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (451.46 -98.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (451.46 -138.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (441.46 -98.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (441.46 -138.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (531.46 -98.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (531.46 -138.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (411.46 -98.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (411.46 -138.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (401.46 -138.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (401.46 -98.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (371.46 -98.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (371.46 -138.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (535.44 0.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (503.94 0.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (472.44 0.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (440.95 0.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (409.45 0.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (377.96 0.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (346.46 0.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (441.46 211.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (381.46 211.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (511.15 211.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (471.77 211.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (446.46 171.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (446.46 131.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (356.46 171.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (356.46 131.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (406.46 171.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (406.46 131.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (501.46 171.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (501.46 131.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (535.44 31.50).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (503.94 31.50).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (472.44 31.50).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (440.95 31.50).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (409.45 31.50).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (377.96 31.50).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (346.46 31.50).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (535.44 63.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (503.94 63.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (472.44 63.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (440.95 63.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (409.45 63.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (377.96 63.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (346.46 63.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (535.44 94.49).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (503.94 94.49).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (472.44 94.49).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (440.95 94.49).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (409.45 94.49).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (377.96 94.49).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (346.46 94.49).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (535.44 125.99).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (503.94 125.99).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (472.44 125.99).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (440.95 125.99).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (409.45 125.99).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (377.96 125.99).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (346.46 125.99).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (535.44 157.48).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (503.94 157.48).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (472.44 157.48).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (440.95 157.48).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (409.45 157.48).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (377.96 157.48).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (346.46 157.48).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (535.44 188.98).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (535.44 220.48).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (472.44 220.48).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (440.95 220.48).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (409.45 220.48).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (377.96 220.48).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (346.46 220.48).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (506.46 396.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (506.46 326.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (506.46 286.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (441.46 251.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (381.46 251.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (361.46 371.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (361.46 411.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (361.46 321.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (361.46 281.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (521.77 251.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (506.77 361.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (546.15 361.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (535.44 251.97).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (472.44 251.97).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (440.95 251.97).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (409.45 251.97).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (377.96 251.97).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (346.46 251.97).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (535.44 283.47).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (472.44 283.47).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (440.95 283.47).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (409.45 283.47).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (377.96 283.47).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (346.46 283.47).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (535.44 314.96).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (472.44 314.96).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (440.95 314.96).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (409.45 314.96).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (377.96 314.96).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (346.46 314.96).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (535.44 346.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (472.44 346.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (440.95 346.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (409.45 346.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (377.96 346.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (346.46 346.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (535.44 377.96).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (472.44 377.96).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (440.95 377.96).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (409.45 377.96).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (377.96 377.96).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (346.46 377.96).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (535.44 409.45).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (472.44 409.45).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (440.95 409.45).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (409.45 409.45).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (377.96 409.45).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (346.46 409.45).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (506.46 436.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (511.15 476.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (471.77 476.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (381.46 441.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (381.46 481.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (441.46 436.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (441.46 476.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (501.46 521.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (501.46 561.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (366.46 521.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (366.46 561.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (406.46 521.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (406.46 561.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (446.46 521.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (446.46 561.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (535.44 440.95).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (472.44 440.95).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (440.95 440.95).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (409.45 440.95).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (377.96 440.95).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (346.46 440.95).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (535.44 472.44).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (472.44 472.44).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (440.95 472.44).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (409.45 472.44).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (377.96 472.44).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (346.46 472.44).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (535.44 503.94).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (535.44 535.44).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (503.94 535.44).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (472.44 535.44).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (440.95 535.44).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (409.45 535.44).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (377.96 535.44).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (346.46 535.44).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (535.44 566.93).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (503.94 566.93).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (472.44 566.93).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (440.95 566.93).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (409.45 566.93).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (377.96 566.93).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (346.46 566.93).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (535.44 598.43).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (503.94 598.43).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (472.44 598.43).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (440.95 598.43).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (409.45 598.43).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (377.96 598.43).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (346.46 598.43).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (535.44 629.92).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (503.94 629.92).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (472.44 629.92).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (440.95 629.92).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (409.45 629.92).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (377.96 629.92).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (346.46 629.92).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (536.46 751.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (536.46 791.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (536.46 791.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (536.46 831.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (496.46 791.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (496.46 831.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (416.46 791.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (416.46 831.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (416.46 791.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (416.46 831.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (496.46 791.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (496.46 831.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (456.46 791.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (456.46 831.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (456.46 791.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (456.46 831.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (376.46 831.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (376.46 791.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (535.44 661.42).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (503.94 661.42).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (472.44 661.42).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (440.95 661.42).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (409.45 661.42).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (377.96 661.42).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (346.46 661.42).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (535.44 692.92).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (503.94 692.92).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (472.44 692.92).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (440.95 692.92).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (409.45 692.92).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (377.96 692.92).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (346.46 692.92).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (361.15 956.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (356.77 1036.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (396.15 1036.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (361.15 906.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (451.46 976.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (451.46 1016.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (491.46 976.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (491.46 1016.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (531.46 1016.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (531.46 976.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (396.46 931.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (396.46 891.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (373.46 1016.86).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_28_12 at (397.80 957.05).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_28_12 at (397.80 931.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_28_12 at (397.80 905.87).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (356.77 1076.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (396.15 1076.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (396.15 1116.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (356.77 1116.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (396.15 1156.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (356.77 1156.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (396.15 1196.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (356.77 1196.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (501.46 1161.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (501.46 1201.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_25_TP at (496.46 1236.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_25_TP at (536.46 1241.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (522.05 1064.06).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (496.46 1064.06).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (470.87 1064.06).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (470.87 1138.86).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (522.05 1138.86).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (373.46 1196.06).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (373.46 1170.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (373.46 1144.86).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (373.46 1119.26).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (373.46 1093.66).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (373.46 1068.06).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (373.46 1042.46).
    WARNING: Null REGULAR-PAD specified for padstack R054X011S at (438.82 1309.10).
    WARNING: Null REGULAR-PAD specified for padstack R054X011S at (458.51 1309.10).
    WARNING: Null REGULAR-PAD specified for padstack R054X011S at (478.19 1309.10).
    WARNING: Null REGULAR-PAD specified for padstack R054X011S at (497.88 1309.10).
    WARNING: Null REGULAR-PAD specified for padstack R054X011S at (517.56 1309.10).
    WARNING: Null REGULAR-PAD specified for padstack R054X011S at (537.25 1309.10).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (386.15 1411.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (386.15 1451.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (401.15 1351.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (361.77 1351.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (401.15 1311.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (361.77 1311.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (431.77 1356.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (471.15 1356.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (501.46 1316.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (501.46 1356.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (541.46 1316.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (541.46 1356.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (531.93 1404.10).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (512.25 1404.10).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (492.56 1404.10).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (459.10 1437.56).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ140NP at (561.46 1506.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (396.46 1496.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (396.46 1536.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (492.56 1608.82).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (512.25 1608.82).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (531.93 1608.82).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (459.10 1457.25).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (459.10 1476.93).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (459.10 1496.62).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (459.10 1516.30).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (459.10 1535.99).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (459.10 1555.67).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (459.10 1575.36).
    WARNING: Null REGULAR-PAD specified for padstack R054X011S at (537.25 1763.82).
    WARNING: Null REGULAR-PAD specified for padstack R054X011S at (517.56 1763.82).
    WARNING: Null REGULAR-PAD specified for padstack R054X011S at (497.88 1763.82).
    WARNING: Null REGULAR-PAD specified for padstack R054X011S at (478.19 1763.82).
    WARNING: Null REGULAR-PAD specified for padstack R054X011S at (458.51 1763.82).
    WARNING: Null REGULAR-PAD specified for padstack R054X011S at (438.82 1763.82).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (501.46 1816.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (501.46 1856.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (541.46 1816.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (541.46 1856.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (421.77 1761.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (461.15 1761.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD40_35 at (461.46 1686.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD40_35 at (521.46 1686.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD40_35 at (376.46 1836.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD40_35 at (436.46 1836.46).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (363.88 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (403.25 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (442.62 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (481.99 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (521.36 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (363.88 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (403.25 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (442.62 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (481.99 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (521.36 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (718.92 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (679.55 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (640.18 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (600.81 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (561.44 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (718.92 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (679.55 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (640.18 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (600.81 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (561.44 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (626.46 -668.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (626.46 -628.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (706.46 -668.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (706.46 -628.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (666.46 -668.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (666.46 -628.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (751.46 -628.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (751.46 -668.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (706.46 -668.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (706.46 -628.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (666.46 -668.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (666.46 -628.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (751.46 -628.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (751.46 -668.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (586.77 -663.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (626.15 -663.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (586.46 -668.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (586.46 -628.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (696.46 -398.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (576.46 -398.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (656.46 -398.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (696.46 -438.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (696.46 -478.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (576.46 -438.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (576.46 -478.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (656.46 -438.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (656.46 -478.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (616.46 -398.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (616.46 -438.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (616.46 -478.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ_35 at (751.46 -408.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ_35 at (751.46 -458.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (571.86 -531.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (597.46 -531.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (623.06 -531.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (648.66 -531.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (674.26 -531.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (699.86 -531.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (725.46 -531.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (696.46 -358.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (576.46 -358.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (656.46 -358.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (616.46 -358.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (735.31 -315.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (725.46 -305.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (699.86 -305.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (674.26 -305.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (648.66 -305.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (623.06 -305.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (597.46 -305.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (571.86 -305.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (576.46 -98.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (576.46 -138.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (616.46 -98.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (616.46 -138.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (576.46 -98.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (576.46 -138.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (736.46 -98.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (736.46 -138.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (616.46 -138.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (616.46 -98.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (696.46 -138.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (696.46 -98.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (696.46 -138.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (696.46 -98.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (656.46 -138.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (656.46 -98.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (656.46 -138.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (656.46 -98.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (692.92 0.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (661.42 0.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (629.92 0.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (598.43 0.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (566.93 0.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (751.77 211.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (751.77 111.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (751.77 61.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (751.77 161.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (692.92 31.50).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (661.42 31.50).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (629.92 31.50).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (598.43 31.50).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (566.93 31.50).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (692.92 63.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (661.42 63.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (629.92 63.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (598.43 63.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (566.93 63.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (692.92 94.49).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (661.42 94.49).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (629.92 94.49).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (598.43 94.49).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (566.93 94.49).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (692.92 125.99).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (661.42 125.99).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (629.92 125.99).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (598.43 125.99).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (566.93 125.99).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (692.92 157.48).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (661.42 157.48).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (629.92 157.48).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (598.43 157.48).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (566.93 157.48).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (692.92 188.98).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (661.42 188.98).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (629.92 188.98).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (598.43 188.98).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (566.93 188.98).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (692.92 220.48).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (661.42 220.48).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (629.92 220.48).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (598.43 220.48).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (566.93 220.48).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (751.77 251.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (751.77 401.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (751.77 336.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (751.77 296.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (561.15 251.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (692.92 251.97).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (661.42 251.97).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (629.92 251.97).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (598.43 251.97).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (566.93 251.97).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (692.92 283.47).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (661.42 283.47).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (629.92 283.47).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (598.43 283.47).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (566.93 283.47).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (692.92 314.96).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (661.42 314.96).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (629.92 314.96).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (598.43 314.96).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (566.93 314.96).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (692.92 346.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (661.42 346.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (629.92 346.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (598.43 346.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (566.93 346.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (692.92 377.96).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (661.42 377.96).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (629.92 377.96).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (598.43 377.96).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (566.93 377.96).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (692.92 409.45).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (661.42 409.45).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (629.92 409.45).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (598.43 409.45).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (566.93 409.45).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (751.77 441.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (692.92 440.95).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (661.42 440.95).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (629.92 440.95).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (598.43 440.95).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (566.93 440.95).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (692.92 472.44).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (661.42 472.44).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (629.92 472.44).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (598.43 472.44).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (566.93 472.44).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (692.92 503.94).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (661.42 503.94).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (629.92 503.94).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (598.43 503.94).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (566.93 503.94).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (692.92 535.44).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (661.42 535.44).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (629.92 535.44).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (598.43 535.44).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (566.93 535.44).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (692.92 566.93).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (661.42 566.93).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (629.92 566.93).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (598.43 566.93).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (566.93 566.93).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (692.92 598.43).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (661.42 598.43).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (629.92 598.43).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (598.43 598.43).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (566.93 598.43).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (692.92 629.92).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (661.42 629.92).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (629.92 629.92).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (598.43 629.92).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (566.93 629.92).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (576.46 751.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (576.46 791.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (616.77 806.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (656.15 806.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (686.77 806.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (726.15 806.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (576.46 791.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (576.46 831.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (676.77 751.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (716.15 751.46).
    WARNING: Null REGULAR-PAD specified for padstack RE12_50 at (698.19 814.69).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (692.92 661.42).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (661.42 661.42).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (629.92 661.42).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (598.43 661.42).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (566.93 661.42).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (692.92 692.92).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (661.42 692.92).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (629.92 692.92).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (598.43 692.92).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_16 at (566.93 692.92).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (631.15 1006.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (591.77 1006.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (661.77 966.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (701.15 966.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (661.77 926.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (701.15 926.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (661.77 886.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (701.15 886.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (661.77 846.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (701.15 846.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (571.77 846.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (611.15 846.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (571.77 886.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (611.15 886.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (591.77 1046.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (631.15 1046.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (726.15 1011.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (686.77 1011.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (599.46 1016.86).
    WARNING: Null REGULAR-PAD specified for padstack RE12_50 at (698.19 840.28).
    WARNING: Null REGULAR-PAD specified for padstack RE12_50 at (698.19 865.87).
    WARNING: Null REGULAR-PAD specified for padstack RE12_50 at (698.19 891.46).
    WARNING: Null REGULAR-PAD specified for padstack RE12_50 at (698.19 917.05).
    WARNING: Null REGULAR-PAD specified for padstack RE12_50 at (698.19 942.64).
    WARNING: Null REGULAR-PAD specified for padstack RE12_50 at (698.19 968.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (631.15 1156.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (591.77 1156.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (731.15 1101.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (691.77 1101.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (591.77 1116.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (631.15 1116.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (571.77 1196.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (611.15 1196.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (756.77 1206.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_25_TP at (626.46 1246.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_25_TP at (581.46 1241.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (599.46 1042.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (599.46 1068.06).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (599.46 1093.66).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (599.46 1119.26).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (599.46 1144.86).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (599.46 1170.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (599.46 1196.06).
    WARNING: Null REGULAR-PAD specified for padstack RE12_50 at (698.19 1049.69).
    WARNING: Null REGULAR-PAD specified for padstack RE12_50 at (698.19 1075.28).
    WARNING: Null REGULAR-PAD specified for padstack RE12_50 at (698.19 1100.87).
    WARNING: Null REGULAR-PAD specified for padstack RE12_50 at (698.19 1126.46).
    WARNING: Null REGULAR-PAD specified for padstack RE12_50 at (698.19 1152.05).
    WARNING: Null REGULAR-PAD specified for padstack RE12_50 at (698.19 1177.64).
    WARNING: Null REGULAR-PAD specified for padstack RE12_50 at (698.19 1203.23).
    WARNING: Null REGULAR-PAD specified for padstack R054X011S at (556.93 1309.10).
    WARNING: Null REGULAR-PAD specified for padstack R054X011S at (576.62 1309.10).
    WARNING: Null REGULAR-PAD specified for padstack R054X011S at (596.30 1309.10).
    WARNING: Null REGULAR-PAD specified for padstack R054X011S at (615.99 1309.10).
    WARNING: Null REGULAR-PAD specified for padstack R054X011S at (635.67 1309.10).
    WARNING: Null REGULAR-PAD specified for padstack R054X011S at (655.36 1309.10).
    WARNING: Null REGULAR-PAD specified for padstack R054X011S at (675.04 1309.10).
    WARNING: Null REGULAR-PAD specified for padstack R054X011S at (694.73 1309.10).
    WARNING: Null REGULAR-PAD specified for padstack R054X011S at (714.41 1309.10).
    WARNING: Null REGULAR-PAD specified for padstack R054X011S at (734.10 1309.10).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (701.46 1316.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (701.46 1356.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (756.46 1421.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (716.46 1421.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (731.77 1356.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (621.46 1356.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (621.46 1316.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (581.46 1356.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (581.46 1316.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (661.46 1356.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (661.46 1316.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (663.82 1437.56).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (630.36 1404.10).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (610.67 1404.10).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (590.99 1404.10).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (571.30 1404.10).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (551.62 1404.10).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (756.46 1461.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (716.46 1461.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (701.77 1666.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (741.15 1666.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ_35 at (706.46 1611.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ_35 at (756.46 1611.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ_35 at (741.46 1506.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ_35 at (741.46 1556.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (551.62 1608.82).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (571.30 1608.82).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (590.99 1608.82).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (610.67 1608.82).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (630.36 1608.82).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (663.82 1575.36).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (663.82 1555.67).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (663.82 1535.99).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (663.82 1516.30).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (663.82 1496.62).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (663.82 1476.93).
    WARNING: Null REGULAR-PAD specified for padstack SMD12X40 at (663.82 1457.25).
    WARNING: Null REGULAR-PAD specified for padstack R054X011S at (734.10 1763.82).
    WARNING: Null REGULAR-PAD specified for padstack R054X011S at (714.41 1763.82).
    WARNING: Null REGULAR-PAD specified for padstack R054X011S at (694.73 1763.82).
    WARNING: Null REGULAR-PAD specified for padstack R054X011S at (675.04 1763.82).
    WARNING: Null REGULAR-PAD specified for padstack R054X011S at (655.36 1763.82).
    WARNING: Null REGULAR-PAD specified for padstack R054X011S at (635.67 1763.82).
    WARNING: Null REGULAR-PAD specified for padstack R054X011S at (615.99 1763.82).
    WARNING: Null REGULAR-PAD specified for padstack R054X011S at (596.30 1763.82).
    WARNING: Null REGULAR-PAD specified for padstack R054X011S at (576.62 1763.82).
    WARNING: Null REGULAR-PAD specified for padstack R054X011S at (556.93 1763.82).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (726.46 1816.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (726.46 1856.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (621.46 1816.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (621.46 1856.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (726.46 1856.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (726.46 1816.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (626.46 1706.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (626.46 1666.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (586.46 1706.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (586.46 1666.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (701.77 1706.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (741.15 1706.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (681.46 1816.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (681.46 1856.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD40_35 at (661.46 1761.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD40_35 at (721.46 1761.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_25_TP at (686.46 1826.46).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (560.73 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (600.10 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (639.47 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (678.84 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (718.21 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (560.73 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (600.10 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (639.47 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (678.84 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (718.21 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (955.15 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (915.77 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (876.40 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (837.03 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (797.66 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (758.29 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (955.15 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (915.77 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (876.40 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (837.03 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (797.66 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (758.29 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (831.46 -668.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (831.46 -628.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (791.46 -628.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (791.46 -668.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (831.46 -628.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (831.46 -668.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (871.46 -668.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (871.46 -628.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (841.15 -463.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (801.77 -463.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (841.15 -423.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (801.77 -423.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (841.15 -543.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (801.77 -543.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (841.15 -503.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (801.77 -503.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (751.06 -531.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (774.69 -315.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (886.15 -333.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (846.77 -333.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (886.15 -268.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (846.77 -268.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (887.05 -226.14).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (861.46 -226.14).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (835.87 -226.14).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (835.87 -300.94).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (887.05 -300.94).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (887.05 -375.94).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (861.46 -375.94).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (835.87 -375.94).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (835.87 -301.14).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (887.05 -301.14).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (955.87 -226.14).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (955.87 -300.94).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (955.87 -375.94).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (955.87 -301.14).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (751.06 -305.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (831.15 -63.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (791.77 -63.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (831.15 16.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (791.77 16.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (831.15 -23.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (791.77 -23.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (831.15 -103.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (791.77 -103.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (831.15 -143.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (791.77 -143.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (831.15 -63.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (791.77 -63.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (831.15 -23.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (791.77 -23.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (831.15 16.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (791.77 16.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (934.06 -164.13).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (934.06 -138.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (934.06 -112.95).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (934.06 -54.13).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (934.06 -28.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (934.06 -2.95).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (921.15 216.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (881.77 216.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (791.15 211.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (791.15 111.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (791.15 61.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (791.15 161.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (886.77 181.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (926.15 181.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (831.15 211.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (791.77 211.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (926.15 136.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (886.77 136.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (926.15 56.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (886.77 56.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (926.15 136.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (886.77 136.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (926.15 96.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (886.77 96.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (926.15 96.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (886.77 96.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (881.77 256.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (921.15 256.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (791.15 251.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (881.77 256.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (921.15 256.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (831.15 251.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (791.77 251.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (791.15 401.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (791.15 336.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (791.15 296.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (876.15 406.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (836.77 406.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (876.15 366.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (836.77 366.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (876.15 366.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (836.77 366.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (876.15 406.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (836.77 406.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ_35 at (846.46 311.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ_35 at (896.46 311.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ_35 at (846.46 311.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ_35 at (896.46 311.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (791.15 441.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (876.15 446.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (836.77 446.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (866.15 491.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (826.77 491.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (831.15 601.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (791.77 601.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (866.15 491.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (826.77 491.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (831.15 601.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (791.77 601.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (876.15 446.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (836.77 446.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ_35 at (801.46 546.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ_35 at (851.46 546.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ_35 at (801.46 546.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ_35 at (851.46 546.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_71_79 at (971.46 591.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_71_79 at (971.46 491.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_32_36 at (868.46 666.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_32_36 at (804.46 666.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_32_36 at (868.46 736.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_32_36 at (804.46 736.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_32_36 at (868.46 736.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_32_36 at (804.46 736.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_32_36 at (868.46 666.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_32_36 at (804.46 666.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_71_79 at (971.46 691.46).
    WARNING: Null REGULAR-PAD specified for padstack RE12_50 at (788.19 814.69).
    WARNING: Null REGULAR-PAD specified for padstack RE12_50 at (914.73 814.69).
    WARNING: Null REGULAR-PAD specified for padstack RE12_50 at (788.19 968.23).
    WARNING: Null REGULAR-PAD specified for padstack RE12_50 at (788.19 942.64).
    WARNING: Null REGULAR-PAD specified for padstack RE12_50 at (788.19 917.05).
    WARNING: Null REGULAR-PAD specified for padstack RE12_50 at (788.19 891.46).
    WARNING: Null REGULAR-PAD specified for padstack RE12_50 at (788.19 865.87).
    WARNING: Null REGULAR-PAD specified for padstack RE12_50 at (788.19 840.28).
    WARNING: Null REGULAR-PAD specified for padstack RE12_50 at (914.73 968.23).
    WARNING: Null REGULAR-PAD specified for padstack RE12_50 at (914.73 942.64).
    WARNING: Null REGULAR-PAD specified for padstack RE12_50 at (914.73 917.05).
    WARNING: Null REGULAR-PAD specified for padstack RE12_50 at (914.73 891.46).
    WARNING: Null REGULAR-PAD specified for padstack RE12_50 at (914.73 865.87).
    WARNING: Null REGULAR-PAD specified for padstack RE12_50 at (914.73 840.28).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (881.77 1116.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (921.15 1116.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (881.77 1076.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (921.15 1076.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (881.77 1196.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (921.15 1196.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (881.77 1156.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (921.15 1156.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (796.15 1206.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (931.86 1258.46).
    WARNING: Null REGULAR-PAD specified for padstack RE12_50 at (914.73 1203.23).
    WARNING: Null REGULAR-PAD specified for padstack RE12_50 at (914.73 1177.64).
    WARNING: Null REGULAR-PAD specified for padstack RE12_50 at (914.73 1152.05).
    WARNING: Null REGULAR-PAD specified for padstack RE12_50 at (914.73 1126.46).
    WARNING: Null REGULAR-PAD specified for padstack RE12_50 at (914.73 1100.87).
    WARNING: Null REGULAR-PAD specified for padstack RE12_50 at (914.73 1075.28).
    WARNING: Null REGULAR-PAD specified for padstack RE12_50 at (914.73 1049.69).
    WARNING: Null REGULAR-PAD specified for padstack R054X011S at (813.82 1388.82).
    WARNING: Null REGULAR-PAD specified for padstack R054X011S at (813.82 1408.51).
    WARNING: Null REGULAR-PAD specified for padstack R054X011S at (813.82 1428.19).
    WARNING: Null REGULAR-PAD specified for padstack R054X011S at (813.82 1447.88).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (786.77 1296.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (826.15 1296.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (786.77 1256.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (826.15 1256.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (821.46 1446.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (771.15 1356.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ_35 at (966.46 1271.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ_35 at (916.46 1271.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (952.46 1353.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (926.86 1353.46).
    WARNING: Null REGULAR-PAD specified for padstack R054X011S at (813.82 1467.56).
    WARNING: Null REGULAR-PAD specified for padstack R054X011S at (813.82 1487.25).
    WARNING: Null REGULAR-PAD specified for padstack R054X011S at (813.82 1506.93).
    WARNING: Null REGULAR-PAD specified for padstack R054X011S at (813.82 1526.62).
    WARNING: Null REGULAR-PAD specified for padstack R054X011S at (813.82 1546.30).
    WARNING: Null REGULAR-PAD specified for padstack R054X011S at (813.82 1565.99).
    WARNING: Null REGULAR-PAD specified for padstack R054X011S at (813.82 1585.67).
    WARNING: Null REGULAR-PAD specified for padstack R054X011S at (813.82 1605.36).
    WARNING: Null REGULAR-PAD specified for padstack R054X011S at (813.82 1625.04).
    WARNING: Null REGULAR-PAD specified for padstack R054X011S at (813.82 1644.73).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (821.46 1486.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (836.46 1556.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (836.46 1516.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (796.46 1556.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (796.46 1516.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (796.77 1631.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (836.15 1631.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (796.77 1591.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (836.15 1591.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ_35 at (926.46 1566.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_25_TP at (861.46 1646.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_25_TP at (901.46 1651.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (931.86 1484.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (926.86 1579.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (952.46 1579.46).
    WARNING: Null REGULAR-PAD specified for padstack R054X011S at (813.82 1664.41).
    WARNING: Null REGULAR-PAD specified for padstack R054X011S at (813.82 1684.10).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (846.46 1816.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (846.46 1856.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (806.46 1816.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (806.46 1856.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (766.46 1816.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (766.46 1856.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (806.46 1856.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (806.46 1816.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (766.46 1856.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (766.46 1816.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (886.46 1856.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (886.46 1816.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (846.46 1856.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (846.46 1816.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (886.46 1816.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (886.46 1856.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD40_35 at (861.46 1746.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD40_35 at (861.46 1686.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD40_35 at (796.46 1686.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD40_35 at (796.46 1746.46).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (757.58 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (796.95 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (836.32 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (875.69 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (915.06 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (954.43 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (757.58 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (796.95 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (836.32 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (875.69 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (915.06 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (954.43 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (1152.00 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (1112.63 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (1073.26 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (1033.89 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (994.52 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (1152.00 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (1112.63 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (1073.26 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (1033.89 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (994.52 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1116.46 -628.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1116.46 -668.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1156.46 -628.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1156.46 -668.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1006.15 -333.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (966.77 -333.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1126.15 -333.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1086.77 -333.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1006.15 -268.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (966.77 -268.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1126.15 -268.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1086.77 -268.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (1127.05 -375.94).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (1101.46 -375.94).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (1075.87 -375.94).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (1075.87 -301.14).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (1127.05 -301.14).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (1007.05 -226.14).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (981.46 -226.14).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (1007.05 -300.94).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (1127.05 -226.14).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (1101.46 -226.14).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (1075.87 -226.14).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (1075.87 -300.94).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (1127.05 -300.94).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (1007.05 -375.94).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (981.46 -375.94).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (1007.05 -301.14).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1095.00 -164.69).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1095.00 -125.31).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (976.46 -53.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (976.46 -13.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (976.46 -163.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (976.46 -123.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1041.46 -163.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1041.46 -123.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1041.46 -53.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1041.46 -13.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1146.46 -8.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (1083.86 -164.13).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (1083.86 -138.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (1083.86 -112.95).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (1009.06 -112.95).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (1009.06 -164.13).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (1083.86 -54.13).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (1083.86 -28.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (1083.86 -2.95).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (1009.06 -2.95).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (1009.06 -54.13).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (1008.86 -112.95).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (1008.86 -164.13).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (1008.86 -2.95).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (1008.86 -54.13).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1141.15 211.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1101.77 211.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1141.15 171.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1101.77 171.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1021.46 81.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1021.46 121.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1086.46 81.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1086.46 121.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1146.46 31.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (979.06 80.87).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (979.06 106.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (979.06 132.05).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (1053.86 132.05).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (1053.86 80.87).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (1128.86 80.87).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (1128.86 106.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (1128.86 132.05).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (1054.06 132.05).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (1054.06 80.87).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1051.46 246.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1051.46 286.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1006.15 326.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (966.77 326.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1051.46 311.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1051.46 351.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD40_35 at (1106.46 266.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD40_35 at (1106.46 326.46).
    WARNING: Null REGULAR-PAD specified for padstack RECT35X45 at (999.37 266.18).
    WARNING: Null REGULAR-PAD specified for padstack RECT35X45 at (1103.55 266.18).
    WARNING: Null REGULAR-PAD specified for padstack RECT35X45 at (999.37 326.74).
    WARNING: Null REGULAR-PAD specified for padstack RECT35X45 at (1103.55 326.74).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1116.46 511.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1116.46 471.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_71_79 at (1136.81 591.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_71_79 at (1136.81 491.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_25_TP at (1066.46 471.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1151.15 801.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1111.77 801.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1146.46 741.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1146.46 701.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1041.77 771.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1081.15 771.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1101.46 681.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1101.46 721.15).
    WARNING: Null REGULAR-PAD specified for padstack RECT25X20 at (1056.46 671.46).
    WARNING: Null REGULAR-PAD specified for padstack RECT25X20 at (1056.46 711.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_71_79 at (1136.81 691.46).
    WARNING: Null REGULAR-PAD specified for padstack RE12_50 at (1004.73 814.69).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1111.15 891.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1071.77 891.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1026.15 866.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (986.77 866.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1026.15 976.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (986.77 976.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1026.15 936.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (986.77 936.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1111.15 851.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1071.77 851.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1111.15 931.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1071.77 931.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (966.77 1026.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1006.15 1026.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1071.46 1046.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_32_36 at (1126.46 1019.46).
    WARNING: Null REGULAR-PAD specified for padstack RE12_50 at (1004.73 840.28).
    WARNING: Null REGULAR-PAD specified for padstack RE12_50 at (1004.73 865.87).
    WARNING: Null REGULAR-PAD specified for padstack RE12_50 at (1004.73 891.46).
    WARNING: Null REGULAR-PAD specified for padstack RE12_50 at (1004.73 917.05).
    WARNING: Null REGULAR-PAD specified for padstack RE12_50 at (1004.73 942.64).
    WARNING: Null REGULAR-PAD specified for padstack RE12_50 at (1004.73 968.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1071.46 1146.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1071.46 1186.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1031.46 1146.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1031.46 1186.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1071.46 1086.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1126.46 1166.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1126.46 1126.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_32_36 at (1126.46 1083.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_32_36 at (1126.46 1204.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (957.46 1258.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (983.06 1258.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (1008.66 1258.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (1034.26 1258.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (1059.86 1258.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (1085.46 1258.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (1111.06 1258.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_32_36 at (1126.46 1268.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (1106.06 1353.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (1080.46 1353.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (1054.86 1353.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (1029.26 1353.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (1003.66 1353.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (978.06 1353.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1156.46 1581.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1156.46 1541.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ_35 at (976.46 1566.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (1111.06 1484.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (1085.46 1484.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (1059.86 1484.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (1034.26 1484.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (1008.66 1484.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (983.06 1484.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (957.46 1484.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (978.06 1579.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (1003.66 1579.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (1029.26 1579.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (1054.86 1579.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (1080.46 1579.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (1106.06 1579.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1151.46 1726.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1151.46 1686.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1136.46 1856.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1136.46 1816.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1131.46 1856.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1131.46 1816.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1171.46 1856.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1171.46 1816.77).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (993.80 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (1033.17 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (1072.54 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (1111.91 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (1151.28 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (993.80 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (1033.17 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (1072.54 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (1111.91 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (1151.28 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (1348.85 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (1309.48 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (1270.11 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (1230.74 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (1191.37 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (1348.85 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (1309.48 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (1270.11 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (1230.74 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (1191.37 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1196.46 -628.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1196.46 -668.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1276.46 -668.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1276.46 -628.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1356.46 -668.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1356.46 -628.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1236.46 -628.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1236.46 -668.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1316.46 -628.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1316.46 -668.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1250.04 -434.13).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_60_18 at (1348.46 -518.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_60_18 at (1348.46 -468.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_60_18 at (1348.46 -418.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1221.46 -423.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1221.46 -463.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ_35 at (1271.46 -418.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ_35 at (1271.46 -468.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1250.04 -207.75).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1250.04 -239.25).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1250.04 -270.74).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_60_18 at (1348.46 -368.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_60_18 at (1348.46 -318.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_60_18 at (1348.46 -268.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_60_18 at (1348.46 -218.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1291.15 -368.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1251.77 -368.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1251.77 -218.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1291.15 -218.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1250.04 -18.78).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1250.04 -50.27).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1250.04 -81.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1250.04 -113.26).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1250.04 -144.76).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1250.04 -176.26).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_60_18 at (1348.46 -168.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_60_18 at (1348.46 -118.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_60_18 at (1348.46 -68.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1276.46 -108.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1276.46 -68.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1276.46 -128.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1276.46 -168.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1250.04 201.70).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1250.04 170.20).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1250.04 138.70).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1250.04 107.21).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1250.04 75.71).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1250.04 44.22).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1250.04 12.72).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_60_18 at (1348.46 31.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_60_18 at (1348.46 81.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_60_18 at (1348.46 131.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_60_18 at (1348.46 181.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1291.15 181.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1251.77 181.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1216.46 131.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1216.46 91.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ_35 at (1271.46 131.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ_35 at (1271.46 81.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1250.04 390.67).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1250.04 359.18).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1250.04 327.68).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1250.04 296.18).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1250.04 264.69).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1250.04 233.19).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_60_18 at (1348.46 231.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_60_18 at (1348.46 281.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_60_18 at (1348.46 331.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_60_18 at (1348.46 381.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1251.77 331.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1291.15 331.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1281.46 421.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1281.46 381.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1250.04 611.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1250.04 579.65).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1250.04 548.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1250.04 516.66).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1250.04 485.16).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1250.04 453.66).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1250.04 422.17).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_60_18 at (1348.46 431.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_60_18 at (1348.46 481.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1336.77 616.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1376.15 616.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1236.77 601.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1276.15 601.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1281.46 441.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1281.46 481.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1250.04 831.62).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1250.04 800.12).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1250.04 768.63).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1250.04 737.13).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1250.04 705.63).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1250.04 674.14).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1250.04 642.64).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1336.77 766.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1376.15 766.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1336.77 716.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1376.15 716.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1336.77 816.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1376.15 816.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1336.77 666.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1376.15 666.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1236.77 641.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1276.15 641.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1271.15 801.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1231.77 801.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_32_36 at (1256.46 689.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_32_36 at (1256.46 753.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1250.04 1020.59).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1250.04 989.10).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1250.04 957.60).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1250.04 926.11).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1250.04 894.61).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1250.04 863.11).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1336.77 916.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1376.15 916.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1336.77 966.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1376.15 966.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1336.77 866.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1376.15 866.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1271.15 846.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1231.77 846.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ_35 at (1256.46 1051.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1250.04 1241.07).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1250.04 1209.57).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1250.04 1178.07).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1250.04 1146.58).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1250.04 1115.08).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1250.04 1083.59).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1250.04 1052.09).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ_35 at (1256.46 1241.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ_35 at (1256.46 1101.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ_35 at (1256.46 1146.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ_35 at (1256.46 1196.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (1353.46 1240.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (1353.46 1214.86).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (1353.46 1189.26).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (1353.46 1163.66).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (1353.46 1138.06).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (1353.46 1112.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (1353.46 1086.86).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1250.04 1430.04).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1250.04 1398.55).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1250.04 1367.05).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1250.04 1335.55).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1250.04 1304.06).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1250.04 1272.56).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ_35 at (1256.46 1291.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (1353.46 1266.06).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (1293.46 1366.26).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (1293.46 1391.86).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (1293.46 1417.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (1293.46 1443.06).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1250.04 1619.02).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1250.04 1587.52).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1250.04 1556.03).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1250.04 1524.53).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1250.04 1493.03).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1250.04 1461.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (1293.46 1468.66).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (1293.46 1494.26).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (1293.46 1519.86).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (1293.46 1545.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (1293.46 1571.06).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (1293.46 1596.66).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1366.46 1816.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1366.46 1856.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1326.46 1816.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1326.46 1856.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1231.46 1686.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1231.46 1726.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1191.46 1686.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1191.46 1726.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1311.46 1686.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1311.46 1726.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1271.46 1686.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1271.46 1726.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1351.46 1726.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1351.46 1686.77).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (1190.65 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (1308.76 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (1348.13 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (1190.65 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (1308.76 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (1348.13 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (1545.70 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (1506.33 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (1466.96 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (1427.59 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (1388.22 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (1545.70 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (1506.33 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (1466.96 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (1427.59 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (1388.22 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_98_189 at (1598.47 -638.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1516.46 -668.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1516.46 -628.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1556.46 -628.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1556.46 -668.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1436.46 -668.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1436.46 -628.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1476.46 -668.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1476.46 -628.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1396.46 -628.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1396.46 -668.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1572.88 -418.38).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1572.88 -223.50).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1572.88 -255.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1572.88 -3.03).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1572.88 -34.52).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1572.88 -66.02).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1572.88 -97.52).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1572.88 -129.01).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1572.88 -160.51).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1572.88 -192.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1572.88 185.95).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1572.88 154.45).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1572.88 122.96).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1572.88 91.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1572.88 59.96).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1572.88 28.47).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1572.88 406.42).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1572.88 374.92).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1572.88 343.43).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1572.88 311.93).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1572.88 280.44).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1572.88 248.94).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1572.88 217.44).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1572.88 626.89).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1572.88 595.40).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1572.88 563.90).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1572.88 532.40).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1572.88 500.91).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1572.88 469.41).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1572.88 437.92).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_50_30 at (1431.46 616.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1572.88 815.87).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1572.88 784.37).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1572.88 752.88).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1572.88 721.38).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1572.88 689.89).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1572.88 658.39).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_50_30 at (1431.46 666.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_50_30 at (1431.46 716.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_50_30 at (1431.46 766.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_50_30 at (1431.46 816.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1572.88 1036.34).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1572.88 1004.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1572.88 973.35).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1572.88 941.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1572.88 910.36).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1572.88 878.86).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1572.88 847.37).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_50_30 at (1431.46 866.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_50_30 at (1431.46 916.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_50_30 at (1431.46 966.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1572.88 1225.32).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1572.88 1193.82).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1572.88 1162.33).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1572.88 1130.83).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1572.88 1099.33).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1572.88 1067.84).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1572.88 1445.79).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1572.88 1414.29).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1572.88 1382.80).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1572.88 1351.30).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1572.88 1319.81).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1572.88 1288.31).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1572.88 1256.81).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ_35 at (1581.46 1366.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (1519.46 1443.06).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (1519.46 1417.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (1519.46 1391.86).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (1519.46 1366.26).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1572.88 1634.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1572.88 1603.27).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1572.88 1571.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1572.88 1540.28).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1572.88 1508.78).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_20_79 at (1572.88 1477.29).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1511.15 1656.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1471.77 1656.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (1519.46 1596.66).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (1519.46 1571.06).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (1519.46 1545.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (1519.46 1519.86).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (1519.46 1494.26).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (1519.46 1468.66).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_98_189 at (1598.47 1821.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1486.46 1816.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1486.46 1856.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1446.46 1816.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1446.46 1856.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1401.46 1756.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1401.46 1716.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1481.46 1756.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1481.46 1716.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1441.46 1756.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1441.46 1716.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1406.46 1856.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1406.46 1816.77).
    WARNING: Null REGULAR-PAD specified for padstack RE36X48 at (1541.96 1831.46).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (1387.50 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (1426.87 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (1466.24 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (1505.61 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (1544.98 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (1387.50 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (1426.87 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (1466.24 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (1505.61 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (1544.98 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (1703.18 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (1663.81 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (1624.44 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (1585.07 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (1703.18 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (1663.81 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (1624.44 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (1585.07 -862.49).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1611.46 -628.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1611.46 -668.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_60_18 at (1754.46 -418.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_60_18 at (1754.46 -468.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_60_18 at (1754.46 -518.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ_35 at (1740.00 -460.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ_35 at (1790.00 -460.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_60_18 at (1754.46 -218.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_60_18 at (1754.46 -268.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_60_18 at (1754.46 -318.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_60_18 at (1754.46 -368.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_60_18 at (1754.46 -68.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_60_18 at (1754.46 -118.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_60_18 at (1754.46 -168.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1686.77 11.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1726.15 11.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1691.46 -113.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1691.46 -73.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1686.77 -33.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1726.15 -33.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_60_18 at (1754.46 181.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_60_18 at (1754.46 131.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_60_18 at (1754.46 81.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_60_18 at (1754.46 31.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1686.77 91.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1726.15 91.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1741.46 171.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1741.46 131.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1686.77 51.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1726.15 51.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1696.46 211.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1696.46 131.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1696.46 171.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_60_18 at (1754.46 381.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_60_18 at (1754.46 331.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_60_18 at (1754.46 281.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_60_18 at (1754.46 231.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1696.46 251.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1696.46 306.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1696.46 346.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_60_18 at (1754.46 481.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_60_18 at (1754.46 431.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1696.46 536.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1696.46 576.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1691.46 436.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1691.46 476.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_50_30 at (1673.46 616.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_95_105 at (1813.86 872.14).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1736.77 646.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1776.15 646.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1736.77 691.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1776.15 691.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1736.77 736.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1776.15 736.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1736.77 781.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1776.15 781.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1736.77 826.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1776.15 826.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1691.46 781.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1691.46 821.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_50_30 at (1673.46 816.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_50_30 at (1673.46 766.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_50_30 at (1673.46 716.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_50_30 at (1673.46 666.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1735.31 950.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1774.69 950.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1691.46 1011.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1691.46 971.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ30 at (1762.50 1000.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_50_30 at (1673.46 966.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_50_30 at (1673.46 916.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_50_30 at (1673.46 866.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1741.15 1121.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1701.77 1121.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1741.15 1081.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1701.77 1081.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1691.46 1066.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1691.46 1106.15).
    WARNING: Null REGULAR-PAD specified for padstack RECT80X90 at (1781.46 1261.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ_35 at (1716.46 1226.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (1629.46 1086.86).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (1629.46 1112.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (1629.46 1138.06).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (1629.46 1163.66).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (1629.46 1189.26).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (1629.46 1214.86).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (1629.46 1240.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1696.77 1326.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1736.15 1326.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1646.46 1441.77).
    WARNING: Null REGULAR-PAD specified for padstack RECT80X90 at (1781.46 1391.46).
    WARNING: Null REGULAR-PAD specified for padstack RECT80X90 at (1741.46 1436.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ_35 at (1631.46 1366.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ_35 at (1716.46 1276.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_65_13 at (1629.46 1266.06).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1646.46 1481.15).
    WARNING: Null REGULAR-PAD specified for padstack RECT80X90 at (1741.46 1566.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_105_100 at (1751.46 1581.46).
    WARNING: Null REGULAR-PAD specified for padstack RE36X48 at (1741.46 1676.96).
    WARNING: Null REGULAR-PAD specified for padstack RE36X48 at (1741.46 1805.96).
    WARNING: Null REGULAR-PAD specified for padstack RE36X48 at (1670.96 1831.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD40_35 at (1656.46 1716.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD40_35 at (1596.46 1716.46).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (1584.35 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (1623.72 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (1663.09 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FB at (1702.46 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (1584.35 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (1623.72 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (1663.09 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD28X166_FT at (1702.46 2050.41).
    WARNING: Null REGULAR-PAD specified for padstack PAD50X100 at (1902.52 -630.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1865.31 -405.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1904.69 -405.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1810.00 -480.31).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1810.00 -519.69).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_30_16 at (1908.66 -458.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_30_16 at (1908.66 -508.54).
    WARNING: Null REGULAR-PAD specified for padstack PAD50X100 at (1902.52 -430.00).
    WARNING: Null REGULAR-PAD specified for padstack PAD50X100 at (1902.52 -530.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_30_16 at (1908.66 -223.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_30_16 at (1908.66 -273.54).
    WARNING: Null REGULAR-PAD specified for padstack PAD50X100 at (1902.52 -225.00).
    WARNING: Null REGULAR-PAD specified for padstack PAD50X100 at (1902.52 -325.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1865.31 -170.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1904.69 -170.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1816.46 -113.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1816.46 -73.85).
    WARNING: Null REGULAR-PAD specified for padstack PAD50X100 at (1902.52 -15.00).
    WARNING: Null REGULAR-PAD specified for padstack PAD50X100 at (1902.52 -125.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1816.46 76.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1816.46 36.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ_35 at (1826.46 81.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ_35 at (1826.46 31.46).
    WARNING: Null REGULAR-PAD specified for padstack PAD50X100 at (1902.52 185.00).
    WARNING: Null REGULAR-PAD specified for padstack PAD50X100 at (1902.52 85.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1905.31 275.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1944.69 275.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_95_105 at (1823.86 567.14).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1821.46 436.77).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1821.46 476.15).
    WARNING: Null REGULAR-PAD specified for padstack S_RCT_1-55_X_0-60 at (1951.46 485.16).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_105_100 at (1856.46 641.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_30_50 at (1856.46 548.96).
    WARNING: Null REGULAR-PAD specified for padstack S_RCT_1-55_X_0-60 at (1951.46 697.76).
    WARNING: Null REGULAR-PAD specified for padstack SMD80_140 at (1934.16 981.52).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ30 at (1817.50 1000.00).
    WARNING: Null REGULAR-PAD specified for padstack RE20X91 at (1934.16 1233.88).
    WARNING: Null REGULAR-PAD specified for padstack RE20X91 at (1934.16 1203.17).
    WARNING: Null REGULAR-PAD specified for padstack RE20X91 at (1934.16 1172.46).
    WARNING: Null REGULAR-PAD specified for padstack RE20X91 at (1934.16 1141.75).
    WARNING: Null REGULAR-PAD specified for padstack RE20X91 at (1934.16 1111.04).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1795.31 1055.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (1834.69 1055.00).
    WARNING: Null REGULAR-PAD specified for padstack RE36X48 at (1811.46 1240.96).
    WARNING: Null REGULAR-PAD specified for padstack RE36X48 at (1811.46 1111.96).
    WARNING: Null REGULAR-PAD specified for padstack SMD40_50 at (1908.96 1211.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD30_50 at (1978.96 1211.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD30_50 at (1978.96 1111.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD30_50 at (1903.96 1111.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD80_140 at (1934.16 1363.40).
    WARNING: Null REGULAR-PAD specified for padstack S_RCT_1-55_X_0-60 at (1995.16 1431.46).
    WARNING: Null REGULAR-PAD specified for padstack S_RCT_1-55_X_0-60 at (1995.16 1581.46).
    WARNING: Null REGULAR-PAD specified for padstack S_RCT_1-55_X_0-60 at (1995.16 1531.46).
    WARNING: Null REGULAR-PAD specified for padstack S_RCT_1-55_X_0-60 at (1995.16 1481.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_30_50 at (1843.96 1581.46).
    WARNING: Null REGULAR-PAD specified for padstack RECT31X35 at (1964.06 1810.83).
    WARNING: Null REGULAR-PAD specified for padstack PAD50X100 at (2052.52 -630.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_30_16 at (2184.26 -508.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_30_16 at (2184.26 -458.54).
    WARNING: Null REGULAR-PAD specified for padstack PAD50X100 at (2052.52 -430.00).
    WARNING: Null REGULAR-PAD specified for padstack PAD50X100 at (2052.52 -530.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_30_16 at (2184.26 -273.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_30_16 at (2184.26 -223.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (2197.05 -390.94).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (2171.46 -390.94).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (2145.87 -390.94).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (2145.87 -316.14).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (2197.05 -316.14).
    WARNING: Null REGULAR-PAD specified for padstack PAD50X100 at (2052.52 -225.00).
    WARNING: Null REGULAR-PAD specified for padstack PAD50X100 at (2052.52 -325.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (2196.15 -48.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (2156.77 -48.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (2197.05 -155.94).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (2171.46 -155.94).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (2145.87 -155.94).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (2145.87 -81.14).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_16_20 at (2197.05 -81.14).
    WARNING: Null REGULAR-PAD specified for padstack PAD50X100 at (2052.52 -15.00).
    WARNING: Null REGULAR-PAD specified for padstack PAD50X100 at (2052.52 -125.00).
    WARNING: Null REGULAR-PAD specified for padstack PAD50X100 at (2052.52 185.00).
    WARNING: Null REGULAR-PAD specified for padstack PAD50X100 at (2052.52 85.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_95_120 at (2099.46 300.60).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (2160.00 310.31).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (2160.00 349.69).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ30 at (2188.96 276.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_95_120 at (2205.75 562.33).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_95_120 at (2089.46 605.60).
    WARNING: Null REGULAR-PAD specified for padstack S_RCT_1-55_X_0-60 at (2001.46 485.16).
    WARNING: Null REGULAR-PAD specified for padstack S_RCT_1-55_X_0-60 at (2051.46 485.16).
    WARNING: Null REGULAR-PAD specified for padstack S_RCT_1-55_X_0-60 at (2101.46 485.16).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_95_120 at (2195.75 867.33).
    WARNING: Null REGULAR-PAD specified for padstack S_RCT_1-55_X_0-60 at (2101.46 697.76).
    WARNING: Null REGULAR-PAD specified for padstack S_RCT_1-55_X_0-60 at (2051.46 697.76).
    WARNING: Null REGULAR-PAD specified for padstack S_RCT_1-55_X_0-60 at (2001.46 697.76).
    WARNING: Null REGULAR-PAD specified for padstack SMD80_140 at (2109.24 981.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (2084.69 860.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (2045.31 860.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_31_35 at (2134.46 1031.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_31_35 at (2188.46 1031.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD40_35 at (2021.46 946.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD40_35 at (2021.46 1006.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ30 at (2032.50 880.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ30 at (2087.50 880.00).
    WARNING: Null REGULAR-PAD specified for padstack SMD250_50 at (2151.46 1173.96).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_31_35 at (2148.46 1251.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_RT_31_35 at (2094.46 1251.46).
    WARNING: Null REGULAR-PAD specified for padstack RECT31X35 at (2114.06 1102.09).
    WARNING: Null REGULAR-PAD specified for padstack RECT31X35 at (2188.86 1102.09).
    WARNING: Null REGULAR-PAD specified for padstack RECT31X35 at (2151.46 1180.83).
    WARNING: Null REGULAR-PAD specified for padstack SMD80_140 at (2109.24 1366.46).
    WARNING: Null REGULAR-PAD specified for padstack S_RCT_1-55_X_0-60 at (2207.76 1431.46).
    WARNING: Null REGULAR-PAD specified for padstack S_RCT_1-55_X_0-60 at (2207.76 1481.46).
    WARNING: Null REGULAR-PAD specified for padstack S_RCT_1-55_X_0-60 at (2207.76 1531.46).
    WARNING: Null REGULAR-PAD specified for padstack S_RCT_1-55_X_0-60 at (2207.76 1581.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (2091.46 1796.15).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (2091.46 1756.77).
    WARNING: Null REGULAR-PAD specified for padstack RECT31X35 at (2038.86 1810.83).
    WARNING: Null REGULAR-PAD specified for padstack RECT31X35 at (2001.46 1732.09).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_40_GFU at (2386.46 -608.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_40_GFU at (2386.46 -608.54).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (2226.46 -473.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (2226.46 -433.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (2226.46 -233.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (2226.46 -193.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (2246.46 -318.85).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_20 at (2246.46 -358.23).
    WARNING: Null REGULAR-PAD specified for padstack SMD_SQ30 at (2243.96 276.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_40_GFU at (2386.46 1781.46).
    WARNING: Null REGULAR-PAD specified for padstack SMD_CR_40_GFU at (2386.46 1781.46).

    ERROR: aborting film - Shape with first seg=(-1218.54 556.46) [layer=TOP]
	has a void with extents [(-1117.55 616.94) (-1035.02 659.98)] that touches
	another shape with first seg=(-1118.54 651.46). Manually resolve problem.

    ERROR: aborting film - artwork will not be generated!
 Error in PLACEMENT--halting output.  Artwork file not generated.
 *** ERROR with PLACEMENT




================================================================
     PROCESSING FILM < TOP_PRINT >
     TO FILE < D:/8309 Rev.B/brd/TOP_PRINT.art > ...
================================================================

  FILM PARAMETERS :
  ---------------------------------------------------------
  Undefined line width                0.00
  Mirror code                         NONE
  Rotate angle                        NONE
  Offset x:                           0.00
  Offset y:                           0.00
  Plot negative                       NO
  Suppress unconnected internal pads  NO



  APERTURES USED:
  ---------------------------------------------------------
  TYPE       SIZE/NAME                   ROT   MIRROR MODE 
  ---------------------------------------------------------
  CIRCLE     0.00394                                  DARK 
  CIRCLE     0.00400                                  DARK 
  CIRCLE     0.00500                                  DARK 
  CIRCLE     0.00591                                  DARK 
  CIRCLE     0.00598                                  DARK 
  CIRCLE     0.00600                                  DARK 
  CIRCLE     0.00700                                  DARK 
  CIRCLE     0.00787                                  DARK 
  CIRCLE     0.00800                                  DARK 
  CIRCLE     0.00984                                  DARK 
  CIRCLE     0.01000                                  DARK 
  CIRCLE     0.01500                                  DARK 
  CIRCLE     0.01600                                  DARK 
  CIRCLE     0.01800                                  DARK 
  CIRCLE     0.01969                                  DARK 
  CIRCLE     0.02000                                  DARK 
  CIRCLE     0.02362                                  DARK 
  CIRCLE     0.03000                                  DARK 
  CIRCLE     0.03543                                  DARK 
  CIRCLE     0.03937                                  DARK 
  CIRCLE     0.04000                                  DARK 
  CIRCLE     0.04330                                  DARK 
  CIRCLE     0.05000                                  DARK 
  CIRCLE     0.05200                                  DARK 
  CIRCLE     0.06100                                  DARK 
  CIRCLE     0.06299                                  DARK 
  CIRCLE     0.12598                                  DARK 
  CIRCLE     0.15000                                  DARK 
  SQUARE     0.03000                     0.000 NO     DARK 
  SQUARE     0.14000                     0.000 NO     DARK 
  RECTANGLE  0.01200     x 0.04000       0.000 NO     DARK 
  RECTANGLE  0.01200     x 0.04000      90.000 NO     DARK 
  RECTANGLE  0.01200     x 0.05000      90.000 NO     DARK 
  RECTANGLE  0.01575     x 0.01969       0.000 NO     DARK 
  RECTANGLE  0.01575     x 0.01969      90.000 NO     DARK 
  RECTANGLE  0.01969     x 0.09055      90.000 NO     DARK 
  RECTANGLE  0.02000     x 0.09055      90.000 NO     DARK 
  RECTANGLE  0.02500     x 0.02000       0.000 NO     DARK 
  RECTANGLE  0.02799     x 0.16598       0.000 NO     DARK 
  RECTANGLE  0.02800     x 0.01200       0.000 NO     DARK 
  RECTANGLE  0.03000     x 0.05000       0.000 NO     DARK 
  RECTANGLE  0.03100     x 0.03500      90.000 NO     DARK 
  RECTANGLE  0.03200     x 0.03600       0.000 NO     DARK 
  RECTANGLE  0.03200     x 0.03600      90.000 NO     DARK 
  RECTANGLE  0.03500     x 0.03500       0.000 NO     DARK 
  RECTANGLE  0.03500     x 0.03500      90.000 NO     DARK 
  RECTANGLE  0.03500     x 0.04500       0.000 NO     DARK 
  RECTANGLE  0.03600     x 0.04800       0.000 NO     DARK 
  RECTANGLE  0.03600     x 0.04800      90.000 NO     DARK 
  RECTANGLE  0.04000     x 0.03500       0.000 NO     DARK 
  RECTANGLE  0.04000     x 0.03500      90.000 NO     DARK 
  RECTANGLE  0.04000     x 0.05000       0.000 NO     DARK 
  RECTANGLE  0.04400     x 0.03200      90.000 NO     DARK 
  RECTANGLE  0.04400     x 0.07200      90.000 NO     DARK 
  RECTANGLE  0.05000     x 0.03000       0.000 NO     DARK 
  RECTANGLE  0.05000     x 0.10000      90.000 NO     DARK 
  RECTANGLE  0.05000     x 0.12500      90.000 NO     DARK 
  RECTANGLE  0.05906     x 0.07874      90.000 NO     DARK 
  RECTANGLE  0.06000     x 0.01800       0.000 NO     DARK 
  RECTANGLE  0.06102     x 0.02362       0.000 NO     DARK 
  RECTANGLE  0.06500     x 0.01300       0.000 NO     DARK 
  RECTANGLE  0.06500     x 0.01300      90.000 NO     DARK 
  RECTANGLE  0.07100     x 0.07900      90.000 NO     DARK 
  RECTANGLE  0.07874     x 0.09900      90.000 NO     DARK 
  RECTANGLE  0.08000     x 0.09000       0.000 NO     DARK 
  RECTANGLE  0.08000     x 0.09000      90.000 NO     DARK 
  RECTANGLE  0.08000     x 0.14000      90.000 NO     DARK 
  RECTANGLE  0.09500     x 0.10500       0.000 NO     DARK 
  RECTANGLE  0.09500     x 0.12000       0.000 NO     DARK 
  RECTANGLE  0.10000     x 0.02800      90.000 NO     DARK 
  RECTANGLE  0.12000     x 0.10000       0.000 NO     DARK 
  RECTANGLE  0.25000     x 0.05000      90.000 NO     DARK 
  OBLONG     0.06000     x 0.10800      90.000 NO     DARK 

     TOP_PRINT created.


================================================================
     PROCESSING FILM < BOT_PRINT >
     TO FILE < D:/8309 Rev.B/brd/BOT_PRINT.art > ...
================================================================

  FILM PARAMETERS :
  ---------------------------------------------------------
  Undefined line width                0.00
  Mirror code                         NONE
  Rotate angle                        NONE
  Offset x:                           0.00
  Offset y:                           0.00
  Plot negative                       NO
  Suppress unconnected internal pads  NO



  APERTURES USED:
  ---------------------------------------------------------
  TYPE       SIZE/NAME                   ROT   MIRROR MODE 
  ---------------------------------------------------------
  CIRCLE     0.00394                                  DARK 
  CIRCLE     0.00400                                  DARK 
  CIRCLE     0.00500                                  DARK 
  CIRCLE     0.00591                                  DARK 
  CIRCLE     0.00598                                  DARK 
  CIRCLE     0.00600                                  DARK 
  CIRCLE     0.00606                                  DARK 
  CIRCLE     0.00700                                  DARK 
  CIRCLE     0.00787                                  DARK 
  CIRCLE     0.00800                                  DARK 
  CIRCLE     0.00984                                  DARK 
  CIRCLE     0.01000                                  DARK 
  CIRCLE     0.01200                                  DARK 
  CIRCLE     0.01500                                  DARK 
  CIRCLE     0.01600                                  DARK 
  CIRCLE     0.01800                                  DARK 
  CIRCLE     0.01969                                  DARK 
  CIRCLE     0.02000                                  DARK 
  CIRCLE     0.02362                                  DARK 
  CIRCLE     0.02500                                  DARK 
  CIRCLE     0.03000                                  DARK 
  CIRCLE     0.03543                                  DARK 
  CIRCLE     0.03937                                  DARK 
  CIRCLE     0.04000                                  DARK 
  CIRCLE     0.04330                                  DARK 
  CIRCLE     0.05000                                  DARK 
  CIRCLE     0.05200                                  DARK 
  CIRCLE     0.06100                                  DARK 
  CIRCLE     0.06299                                  DARK 
  CIRCLE     0.12598                                  DARK 
  CIRCLE     0.15000                                  DARK 
  SQUARE     0.03000                     0.000 NO     DARK 
  RECTANGLE  0.01000     x 0.03200       0.000 NO     DARK 
  RECTANGLE  0.01200     x 0.05000      90.000 NO     DARK 
  RECTANGLE  0.01575     x 0.01969       0.000 NO     DARK 
  RECTANGLE  0.01575     x 0.01969      90.000 NO     DARK 
  RECTANGLE  0.01969     x 0.07874      90.000 NO     DARK 
  RECTANGLE  0.02500     x 0.02000       0.000 NO     DARK 
  RECTANGLE  0.02500     x 0.02000      90.000 NO     DARK 
  RECTANGLE  0.02700     x 0.01000       0.000 NO     DARK 
  RECTANGLE  0.02700     x 0.01000      90.000 NO     DARK 
  RECTANGLE  0.02799     x 0.16598       0.000 NO     DARK 
  RECTANGLE  0.02800     x 0.07100      90.000 NO     DARK 
  RECTANGLE  0.03000     x 0.01600       0.000 NO     DARK 
  RECTANGLE  0.03000     x 0.05000       0.000 NO     DARK 
  RECTANGLE  0.03000     x 0.05000      90.000 NO     DARK 
  RECTANGLE  0.03100     x 0.03500       0.000 NO     DARK 
  RECTANGLE  0.03100     x 0.03500      90.000 NO     DARK 
  RECTANGLE  0.03200     x 0.03600       0.000 NO     DARK 
  RECTANGLE  0.03200     x 0.03600      90.000 NO     DARK 
  RECTANGLE  0.03500     x 0.03500       0.000 NO     DARK 
  RECTANGLE  0.03500     x 0.03500      90.000 NO     DARK 
  RECTANGLE  0.03500     x 0.04500       0.000 NO     DARK 
  RECTANGLE  0.03937     x 0.00984       0.000 NO     DARK 
  RECTANGLE  0.04000     x 0.03500       0.000 NO     DARK 
  RECTANGLE  0.04000     x 0.03500      90.000 NO     DARK 
  RECTANGLE  0.04000     x 0.05000       0.000 NO     DARK 
  RECTANGLE  0.04000     x 0.07100      90.000 NO     DARK 
  RECTANGLE  0.05400     x 0.01100       0.000 NO     DARK 
  RECTANGLE  0.05400     x 0.01100      90.000 NO     DARK 
  RECTANGLE  0.05500     x 0.06500       0.000 NO     DARK 
  RECTANGLE  0.06000     x 0.11000      90.000 NO     DARK 
  RECTANGLE  0.06102     x 0.02362       0.000 NO     DARK 
  RECTANGLE  0.06102     x 0.02362      90.000 NO     DARK 
  RECTANGLE  0.06500     x 0.01300      90.000 NO     DARK 
  RECTANGLE  0.08000     x 0.09000       0.000 NO     DARK 
  RECTANGLE  0.08000     x 0.09000      90.000 NO     DARK 
  RECTANGLE  0.09800     x 0.06600       0.000 NO     DARK 
  RECTANGLE  0.09843     x 0.18898      90.000 NO     DARK 
  RECTANGLE  0.10000     x 0.17800       0.000 NO     DARK 
  RECTANGLE  0.10500     x 0.10000       0.000 NO     DARK 
  RECTANGLE  0.10500     x 0.10000      90.000 NO     DARK 
  OBLONG     0.06000     x 0.10800      90.000 NO     DARK 

     BOT_PRINT created.


================================================================
     PROCESSING FILM < BOT_ROUTE >
     TO FILE < D:/8309 Rev.B/brd/BOT_ROUTE.art > ...
================================================================

  FILM PARAMETERS :
  ---------------------------------------------------------
  Undefined line width                0.00
  Mirror code                         NONE
  Rotate angle                        NONE
  Offset x:                           0.00
  Offset y:                           0.00
  Plot negative                       NO
  Suppress unconnected internal pads  NO



  APERTURES USED:
  ---------------------------------------------------------
  TYPE       SIZE/NAME                   ROT   MIRROR MODE 
  ---------------------------------------------------------
  CIRCLE     0.00394                                  DARK 
  CIRCLE     0.00400                                  DARK 
  CIRCLE     0.00500                                  DARK 
  CIRCLE     0.00591                                  DARK 
  CIRCLE     0.00598                                  DARK 
  CIRCLE     0.00600                                  DARK 
  CIRCLE     0.00606                                  DARK 
  CIRCLE     0.00700                                  DARK 
  CIRCLE     0.00787                                  DARK 
  CIRCLE     0.00800                                  DARK 
  CIRCLE     0.00984                                  DARK 
  CIRCLE     0.01000                                  DARK 
  CIRCLE     0.01200                                  DARK 
  CIRCLE     0.01500                                  DARK 
  CIRCLE     0.01600                                  DARK 
  CIRCLE     0.01800                                  DARK 
  CIRCLE     0.01969                                  DARK 
  CIRCLE     0.02000                                  DARK 
  CIRCLE     0.02362                                  DARK 
  CIRCLE     0.02500                                  DARK 
  CIRCLE     0.03000                                  DARK 
  CIRCLE     0.03543                                  DARK 
  CIRCLE     0.03937                                  DARK 
  CIRCLE     0.04000                                  DARK 
  CIRCLE     0.04330                                  DARK 
  CIRCLE     0.05000                                  DARK 
  CIRCLE     0.05200                                  DARK 
  CIRCLE     0.06100                                  DARK 
  CIRCLE     0.06299                                  DARK 
  CIRCLE     0.12598                                  DARK 
  CIRCLE     0.15000                                  DARK 
  SQUARE     0.03000                     0.000 NO     DARK 
  RECTANGLE  0.01000     x 0.03200       0.000 NO     DARK 
  RECTANGLE  0.01200     x 0.05000      90.000 NO     DARK 
  RECTANGLE  0.01575     x 0.01969       0.000 NO     DARK 
  RECTANGLE  0.01575     x 0.01969      90.000 NO     DARK 
  RECTANGLE  0.01969     x 0.07874      90.000 NO     DARK 
  RECTANGLE  0.02500     x 0.02000       0.000 NO     DARK 
  RECTANGLE  0.02500     x 0.02000      90.000 NO     DARK 
  RECTANGLE  0.02700     x 0.01000       0.000 NO     DARK 
  RECTANGLE  0.02700     x 0.01000      90.000 NO     DARK 
  RECTANGLE  0.02799     x 0.16598       0.000 NO     DARK 
  RECTANGLE  0.02800     x 0.07100      90.000 NO     DARK 
  RECTANGLE  0.03000     x 0.01600       0.000 NO     DARK 
  RECTANGLE  0.03000     x 0.05000       0.000 NO     DARK 
  RECTANGLE  0.03000     x 0.05000      90.000 NO     DARK 
  RECTANGLE  0.03100     x 0.03500       0.000 NO     DARK 
  RECTANGLE  0.03100     x 0.03500      90.000 NO     DARK 
  RECTANGLE  0.03200     x 0.03600       0.000 NO     DARK 
  RECTANGLE  0.03200     x 0.03600      90.000 NO     DARK 
  RECTANGLE  0.03500     x 0.03500       0.000 NO     DARK 
  RECTANGLE  0.03500     x 0.03500      90.000 NO     DARK 
  RECTANGLE  0.03500     x 0.04500       0.000 NO     DARK 
  RECTANGLE  0.03937     x 0.00984       0.000 NO     DARK 
  RECTANGLE  0.04000     x 0.03500       0.000 NO     DARK 
  RECTANGLE  0.04000     x 0.03500      90.000 NO     DARK 
  RECTANGLE  0.04000     x 0.05000       0.000 NO     DARK 
  RECTANGLE  0.04000     x 0.07100      90.000 NO     DARK 
  RECTANGLE  0.05400     x 0.01100       0.000 NO     DARK 
  RECTANGLE  0.05400     x 0.01100      90.000 NO     DARK 
  RECTANGLE  0.05500     x 0.06500       0.000 NO     DARK 
  RECTANGLE  0.06000     x 0.11000      90.000 NO     DARK 
  RECTANGLE  0.06102     x 0.02362       0.000 NO     DARK 
  RECTANGLE  0.06102     x 0.02362      90.000 NO     DARK 
  RECTANGLE  0.06500     x 0.01300      90.000 NO     DARK 
  RECTANGLE  0.08000     x 0.09000       0.000 NO     DARK 
  RECTANGLE  0.08000     x 0.09000      90.000 NO     DARK 
  RECTANGLE  0.09800     x 0.06600       0.000 NO     DARK 
  RECTANGLE  0.09843     x 0.18898      90.000 NO     DARK 
  RECTANGLE  0.10000     x 0.17800       0.000 NO     DARK 
  RECTANGLE  0.10500     x 0.10000       0.000 NO     DARK 
  RECTANGLE  0.10500     x 0.10000      90.000 NO     DARK 
  OBLONG     0.06000     x 0.10800      90.000 NO     DARK 

     BOT_ROUTE created.


================================================================
     PROCESSING FILM < LAYER6 >
     TO FILE < D:/8309 Rev.B/brd/LAYER6.art > ...
================================================================

  FILM PARAMETERS :
  ---------------------------------------------------------
  Undefined line width                6.00
  Mirror code                         NONE
  Rotate angle                        NONE
  Offset x:                           0.00
  Offset y:                           0.00
  Plot negative                       NO
  Suppress unconnected internal pads  NO



  APERTURES USED:
  ---------------------------------------------------------
  TYPE       SIZE/NAME                   ROT   MIRROR MODE 
  ---------------------------------------------------------
  CIRCLE     0.00400                                  DARK 
  CIRCLE     0.00600                                  DARK 
  CIRCLE     0.01000                                  DARK 
  CIRCLE     0.01500                                  DARK 
  CIRCLE     0.01800                                  DARK 
  CIRCLE     0.02000                                  DARK 
  CIRCLE     0.02500                                  DARK 
  CIRCLE     0.03543                                  DARK 
  CIRCLE     0.03937                                  DARK 
  CIRCLE     0.04000                                  DARK 
  CIRCLE     0.04330                                  DARK 
  CIRCLE     0.05000                                  DARK 
  CIRCLE     0.05200                                  DARK 
  CIRCLE     0.06100                                  DARK 
  CIRCLE     0.06299                                  DARK 
  CIRCLE     0.12598                                  DARK 
  CIRCLE     0.15000                                  DARK 
  OBLONG     0.06000     x 0.10800      90.000 NO     DARK 

     LAYER6 created.


================================================================
     PROCESSING FILM < LAYER7 >
     TO FILE < D:/8309 Rev.B/brd/LAYER7.art > ...
================================================================

  FILM PARAMETERS :
  ---------------------------------------------------------
  Undefined line width                6.00
  Mirror code                         NONE
  Rotate angle                        NONE
  Offset x:                           0.00
  Offset y:                           0.00
  Plot negative                       NO
  Suppress unconnected internal pads  NO



  APERTURES USED:
  ---------------------------------------------------------
  TYPE       SIZE/NAME                   ROT   MIRROR MODE 
  ---------------------------------------------------------
  CIRCLE     0.00600                                  DARK 
  CIRCLE     0.01500                                  DARK 
  CIRCLE     0.01800                                  DARK 
  CIRCLE     0.02000                                  DARK 
  CIRCLE     0.03543                                  DARK 
  CIRCLE     0.03937                                  DARK 
  CIRCLE     0.04000                                  DARK 
  CIRCLE     0.04330                                  DARK 
  CIRCLE     0.05000                                  DARK 
  CIRCLE     0.05200                                  DARK 
  CIRCLE     0.06100                                  DARK 
  CIRCLE     0.06299                                  DARK 
  CIRCLE     0.12598                                  DARK 
  CIRCLE     0.15000                                  DARK 
  OBLONG     0.06000     x 0.10800      90.000 NO     DARK 

     LAYER7 created.


------------------------------------------------------
 SUMMARY:
        BOTASSY created with warnings
        LAYER2 created.
        LAYER3 created.
        LAYER4 created.
        BOTMASK created.
        BOTPASTE created.
        BOTSILK created.
        BOTTOM created.
        LAYER5 created.
        TOP created.
        TOPASSY created.
        TOPMASK created.
        TOPPASTE created.
        TOPSILK created.
        FABRICATION created.
        TOP_PLACE created with warnings
    *** ERROR with BOT_PLACE
        TOP_ROUTE created.
    *** ERROR with PLACEMENT
        TOP_PRINT created.
        BOT_PRINT created.
        BOT_ROUTE created.
        LAYER6 created.
        LAYER7 created.

 ARTWORK Error
